For 1990-2009 cars

### Removal Procedure

1. Remove the rear side door trim panel. Refer to Rear Side Door Trim Panel Replacement .
2. Remove the rear side door window belt inner sealing strip. Refer to Rear Side Door Window Inner Sealing Strip Replacement .
3. Remove the rear side door water deflector. Refer to Rear Side Door Water Deflector Replacement .
4. Remove the rear side door frame appliques. Refer to Rear Door Frame Applique Replacement .
5. Lower window to access the window release tab.
6. Remove the rear side window run channel bolts and loosen the window run channel.
7. Depress the window release tab with a flat-bladed tool.
8. Pull the window out of the window regulator guide plate.
9. Slide the window down and out of the primary window run channels.
10. Remove the window through the door belt opening.

### Installation Procedure

1. Install the window by sliding the window into the door through the outside door belt opening.
2. Install the window into the primary window run channels and position into the regulator guide plate.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the rear side window run channel bolts.

Tighten
Tighten the bolts to 8 N·m (71 lb in).

4. Install the rear side door water deflector. Refer to Rear Side Door Water Deflector Replacement .
5. Install the rear side door window belt inner sealing strip. Refer to Rear Side Door Window Inner Sealing Strip Replacement .
6. Install the rear side door trim panel. Refer to Rear Side Door Trim Panel Replacement .
7. Install the rear side door frame appliques. Refer to Rear Door Frame Applique Replacement .
8. Operate the window to inspect the operation.