For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the air inlet grille panel. Refer to Air Inlet Grille Panel Replacement .

1 | Windshield Washer System Module Assembly Bolts (Qty: 3) Notice: Refer to Fastener Notice in the Preface section. Tighten Tighten the bolts in the mandatory sequence as shown to 12 N·m (9 lb ft)
2 | Windshield Washer System Module Assembly Tip

• | Raise the module from the plenum and disconnect the electrical connector from the wiper motor.

• | Re-connect the electrical connector prior to the installation of the wiper washer module back into the plenum.

3 | Windshield Washer Module Assembly Harness
4 | Windshield Washer Module Assembly Harness Rosebud Tip Ensure the rosebud is fastened to the plenum flange to ensure the harness is secure.