For 1990-2009 cars

## Floor Panel Carpet Replacement Front

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the front seats. Refer to Front Seat Replacement - Bucket .
2. Remove the rear seats. Refer to Rear Seat Replacement .
3. Remove the front carpet retainer. Refer to Front Carpet Retainer Replacement .
4. Remove the rear carpet retainer. Refer to Rear Carpet Retainer Replacement .
5. Remove the center console trim panels and the center console. Refer to Console Replacement .

1 | Front Floor Panel Carpet Assembly Tip Remove the floor carpet by pulling the carpet from under the center pillar assemblies and lifting the carpet out of the vehicle.

## Floor Panel Carpet Replacement Rear

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove third row seats.
2. Remove rear quarter lower trim panel. Refer to Quarter Lower Rear Trim Panel Replacement .
3. Remove liftgate door sill plate. Refer to Liftgate Door Sill Plate Replacement .

1 | Rear Floor Panel Carpet Assembly