For 1990-2009 cars

### Removal Procedure

1. Lower the front door window.
2. Remove the front side door trim panel. Refer to Front Side Door Trim Panel Replacement .
3. Remove the front side door window belt inner sealing strip. Refer to Front Side Door Window Belt Inner Sealing Strip Replacement .
4. Starting at one end, carefully pull the window weatherstrip run channel from the door frame.

### Installation Procedure

1. Install the rear side window weatherstrip run channel.

1.1. | Starting at the lower rear corner of the window opening, press the weatherstrip run channel onto the door flange.

1.2. | Ensure the channel is fully secured into the upper corners of the front side door frame.

2. Install the front side door window belt inner sealing strip. Refer to Front Side Door Window Belt Inner Sealing Strip Replacement .
3. Install the front side door trim panel. Refer to Front Side Door Trim Panel Replacement .