For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the floor console. Refer to Console Replacement .

1 | Instrument Panel Lower Brace Bezel Refer to Instrument Panel Lower Brace Bezel Replacement .
2 | Console Trim Panel Assembly Screw (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
3 | Console Trim Panel Assembly - Right
4 | Retainer Clip (Qty: 3)