For 1990-2009 cars

### Removal Procedure

1. Remove the coil spring. Refer to Coil Spring Replacement .
2. Remove the upper and lower rubber insulators from the coil spring.

### Installation Procedure

Important:

• | Spray silicon lubricant on the insulators to aid in installation.

• | Make sure that part number identification tape located on the coil spring is oriented outboard of the vehicle and at the top of the spring.

• | Make sure to fully seat the top and bottom coil spring insulators to the spring.

1. Install the upper and lower rubber insulators to the coil spring.
2. Install the coil spring. Refer to Coil Spring Replacement .