For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Condenser to Radiator Bolts | 9 N·m | 80 lb in
Cooling Fan Motor Bolts | 9 N·m | 80 lb in
Cooling Fan Motor Nuts | 6 N·m | 53 lb in
CRFM Bracket Bolts | 20 N·m | 15 lb ft
Fan Shroud to Radiator Bolts | 9 N·m | 80 lb in
Heater Inlet Housing Bolts | 10 N·m | 89 lb in
Surge Tank to Body Bolts | 9 N·m | 80 lb in
Thermostat Housing Bolts | 10 N·m | 89 lb in
Water Outlet Housing Bolts | 10 N·m | 89 lb in
Water Pump Bolts | 10 N·m | 89 lb in
Water Pump Pulley Bolts | 10 N·m | 89 lb in