For 1990-2009 cars

Application | Specification
--- | ---
Model/PKG | Tire Size | Curb Height
Front Suspension Height (P) | SLF26 and SLG26 | P235/65R16 QKG P235/60R17 QLJ | 818 mm ± 10 mm 823 mm ± 10 mm
Rear Suspension Height (R) | SLF26 and SLG26 | P235/65R16 QKG P235/60R17 QLJ | 832 mm ± 10 mm 836 mm ± 10 mm
Front Suspension Height (Z) | SLF26 and SLG26 | P235/65R16 QKG P235/60R17 QLJ | 18 mm ± 10 mm 18 mm ± 10 mm
Rear Suspension Height (D) | SLF26 and SLG26 | P235/65R16 QKG P235/60R17 QLJ | 42 mm ± 10 mm 42 mm ± 10 mm
The rear suspension D Height is the difference (D=a-b) measured as a horizontal line through the center of the cradle attachment bolt (a) and the center of the knuckle attachment bolt (b). All measurements are taken with a full tank of gas.