For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Disconnect the battery. Refer to Battery Replacement

1 | Underhood Electrical Center/Junction Block Cover Tab (Qty: 2)

#### Procedure

To remove the junction block cover, push in on the two locking tabs located on the rear of the cover and lift. To reinstall, fit together the tabs located on the front of the cover and push down on the cover until the tabs on the rear of the cover (closest to the dash) click into place.

2 | Underhood Electrical Center/Junction Block Power Nut Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

Disconnect the battery positive cable from the junction block by removing the nut.

Tighten
7 N·m (62 lb in)

3 | Underhood Electrical Center/Junction Block Tab (Qty: 6)

#### Procedure

Remove the electrical center/junction block by using a hook-like tool to disengage the tabs.