For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the steering wheel. Refer to Steering Wheel Replacement.
2. Remove the steering column trim covers. Refer to Steering Column Trim Covers Replacement.

1 | Inflatable Restraint Steering Wheel Module Coil Bolt (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 1.5 N·m (13 lb in).
2 | Inflatable Restraint Steering Wheel Module Coil

#### Procedure

1. Disconnect any electrical connectors as needed.
2. A new inflatable restraint steering wheel module coil will be equipped with a yellow tab that should be removed after the steering wheel is installed.