For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the rear seat. Refer to Rear Seat Replacement.
2. Remove the rear seat latch. Refer to Rear Seat Latch Replacement.
3. Remove the rear seat cushion cover and pad. Refer to Rear Seat Cushion Cover and Pad Replacement.

1 | Rear Seat Number 1 Cushion Frame Bolt (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 25 N·m (18 lb ft)
2 | Rear Seat Number 1 Cushion Frame Tip Remove the seat cushion pad from the seat cushion cover.