For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the hood overslam bumpers. Refer to Hood Bumper Replacement .
2. Remove the primary hood latch. Refer to Hood Primary Latch Replacement .
3. Remove the front headlamps. Refer to Headlamp Replacement .

1 | Front Bumper Fascia Support Bolt (Qty: 13) Caution: Refer to Fastener Caution in the Preface section. Tighten 10 N·m (89 lb in)
2 | Front Bumper Fascia Support