For 1990-2009 cars

### Removal Procedure

1. Remove the fuel tank. Refer to Fuel Tank Replacement.
2. Remove the fuel tank fill vent line from the retaining feature built into the tank.
3. Remove the fuel tank fill vent line from the fuel tank clips.

### Installation Procedure

1. Install the fuel tank fill vent line to the fuel tank clips.
2. Install the fuel tank fill vent line to the retaining feature built into the tank.
3. Install the fuel tank. Refer to Fuel Tank Replacement.