For 1990-2009 cars

### Removal Procedure

1. Remove the front side door outside handle. Refer to Front Side Door Outside Handle Replacement .
2. Remove the front side door window run channel. Refer to Front Side Door Window Channel Replacement .
3. Remove the front side door speaker. Refer to Radio Front Side Door Speaker Replacement .
4. Disconnect the mirror electrical connector.
5. Disconnect the 4 electrical connector rosebuds (2 at the mirror and 2 under the speaker).
6. Loosen the 2 rear module bolts.
7. Remove the 4 remaining module bolts.
8. Remove the 3 latch bolts from the door shut face.
9. Disconnect the door harness at the door jamb.
10. Remove the window regulator module from the door.

### Installation Procedure

1. Install the window regulator module into the door.
2. Connect the door harness at the door jamb.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the front side door 3 latch screws to the door shut face.

Tighten the bolts to 10 N·m (89 lb in) .

4. Install the front side door 4 module bolts.

Tighten the bolts to 8 N·m (71 lb in) .

5. Connect the 4 electrical connector rosebuds (2 at the mirror and 2 under the speaker).
6. Connect the mirror electrical connector.
7. Install the front side door speaker. Refer to Radio Front Side Door Speaker Replacement .
8. Install the front door window run channel. Refer to Front Side Door Window Channel Replacement .
9. Install the front door outside handle. Refer to Front Side Door Outside Handle Replacement .