For 1990-2009 cars

### Removal Procedure

1. Loosen the screw in the base of the mirror.
2. Remove the mirror from the mounting pad.
3. Disconnect the rearview mirror wiring harness, if applicable.

### Installation Procedure

1. Install the mirror to the mounting pad.

Notice: Refer to Fastener Notice in the Preface section.

2. Tighten the screw that retains the mirror base to the mounting pad.

Tighten
Tighten the mirror set screw to 2 N·m (18 lb in).

3. Install the rearview mirror wiring harness, if applicable.