For 1990-2009 cars

Connector 1: | X101 Body Harness to the Forward Lamp Harness
Connector 2: | X102 Body Harness to the Battery Cable Harness
Connector 3: | X103 Left Front Wheel Speed Sensor Harness to the Body Harness
Connector 4: | X104 Right Front Wheel Speed Sensor Harness to the Body Harness
Connector 5: | X105 Engine Harness to the Fuel Injector Harness
Connector 6: | X106 Body Harness to the Engine Harness
Connector 7: | X108 Forward Lamp Harness to the Right Cooling Fan Harness
Connector 8: | X109 Forward Lamp Harness to the Left Headlamp Harness
Connector 9: | X110 Forward Lamp Harness to the Right Headlamp Harness
Connector 10: | X202 Console Harness to the Instrument Panel Harness (C69+UUC)
Connector 11: | X203 Console Harness to the Instrument Panel Harness (C69-UUC)
Connector 12: | X204 Instrument Panel Harness to the Body Harness
Connector 13: | X206 Instrument Panel Harness to the Body Harness
Connector 14: | X207 Console Harness to the Instrument Panel Harness (UUC-C69)
Connector 15: | X210 Instrument Panel Harness to the Body Harness
Connector 16: | X214 Passenger Airbag Jumper Harness to the Instrument Panel Harness
Connector 17: | X216 Instrument Panel Harness to the HVAC Harness
Connector 18: | X218 Instrument Panel Harness to the Body Harness
Connector 19: | X219 Body Harness to the Instrument Panel Harness
Connector 20: | X223 Sunload/Ambient Light Sensor Harness to the Instrument Panel Harness
Connector 21: | X226 Instrument Panel Harness to the Shifter Jumper Harness
Connector 22: | X275 Instrument Panel Harness to the Steering Wheel Module Coil Harness
Connector 23: | X276 Instrument Panel Harness to the Steering Wheel Module Coil Harness
Connector 24: | X277 Steering Wheel Controls Harness to the Steering Wheel Module Coil Harness
Connector 25: | X305 Console Harness to the Body Harness
Connector 26: | X307 Body Harness to the Instrument Panel Harness (C69)
Connector 27: | X308 Body Harness to the Power Seat Harness (AG1 -KA1)
Connector 28: | X308 Body Harness to the Driver Seat Harness (KA1)
Connector 29: | X309 Body Harness to the Passenger Seat Harness (-KA1)
Connector 30: | X309 Body Harness to the Passenger Seat Harness (KA1)
Connector 31: | X311 Headliner Harness to the Dome Lamp Harness (UUC)
Connector 32: | X312 Driver Seat Harness to the Power Seat Harness (AG1 +KA1)
Connector 33: | X313 Passenger Presence Harness to the Passenger Seat Harness
Connector 34: | X314 Headliner Harness to the Sunroof Harness (CF5)
Connector 35: | X400 Body Harness to the Chassis Harness
Connector 36: | X403 Body Harness to the Left Tail Lamp Harness
Connector 37: | X404 Body Harness to the Right Tail Lamp Harness
Connector 38: | X406 Body Harness to the Fuel Sender Harness
Connector 39: | X409 Body Harness to the Trailer Jumper Harness (V92)
Connector 40: | X410 Trailer Harness to the Trailer Jumper Harness (V92)
Connector 41: | X412 Headliner Harness to the Instrument Panel Harness (UUC)
Connector 42: | X415 Headliner Harness to the Body Harness
Connector 43: | X417 Headliner Harness to the Body Harness (U3U)
Connector 44: | X419 Body Harness to the Rear HVAC Harness (C69)
Connector 45: | X420 Body Harness to the Left Inflatable Restraint Roof Rail Module Harness (ASF)
Connector 46: | X421 Body Harness to the Right Inflatable Restraint Roof Rail Module Harness (ASF)
Connector 47: | X500 Body Harness to the Left Front Door Harness
Connector 48: | X600 Body Harness to the Right Front Door Harness
Connector 49: | X700 Body Harness to the Left Rear Door Harness
Connector 50: | X800 Body Harness to the Right Rear Door Harness
Connector 51: | X900 Body Harness to the Liftgate Harness
Connector 52: | X901 Body Harness to the Liftgate Harness
Connector 53: | X906 Liftgate Harness to the License Lamp Harness

### X101 Body Harness to the Forward Lamp Harness

#### Connector Part Information

- OEM: 7283-5684-10
- Service: See Catalog
- Description: 8-Way F Receptacle 1.5 Sealed (D-GY)

#### Connector Part Information

- OEM: 7282-5684-10
- Service: See Catalog
- Description: 8-Way M 1.5 Sealed (D-GY)

#### Terminal Part Information

- Pins: 1-4, 7-8
- Terminal/Tray: 7116-4102-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

- Pins: 6
- Terminal/Tray: 7116-4103-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

#### Terminal Part Information

- Pins: 1-4, 7-8
- Terminal/Tray: 7114-4102-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-3 (GY)

- Pins: 6
- Terminal/Tray: 7114-4103-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-3 (GY)

#### X101 Body Harness to the Forward Lamp Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.35 L-GN/BK | 735 | Ambient Air Temperature Sensor Signal (UH9) | 1 | 0.35 L-GN/BK | 735 | Ambient Air Temperature Sensor Signal (UH9)
2 | 0.35 YE | 61 | Low Reference (UH9) | 2 | 0.35 YE | 61 | Low Reference (UH9)
3 | 0.35 TN/OG | 5045 | Low Reference | 3 | 0.35 TN/OG | 5045 | Low Reference
4 | 0.35 YE | 354 | Front End Sensor - Left - Signal | 4 | 0.35 YE | 354 | Front End Sensor - Left - Signal
5 | -- | -- | Not Used | 5 | -- | -- | Not Used
6 | 1.0 BK | 1250 | Ground | 6 | 1.0 BK | 1250 | Ground
7 | 0.35 GY | 5600 | Low Reference | 7 | 0.35 GY | 5600 | Low Reference
8 | 0.35 D-GN | 1409 | Front End Sensor - Right - Signal | 8 | 0.35 D-GN | 1409 | Front End Sensor - Right - Signal

### X102 Body Harness to the Battery Cable Harness

#### Connector Part Information

- OEM: 7283-5548-30
- Service: 88953306
- Description: 2-Way F YESC Weather Pack (BK)

#### Connector Part Information

- OEM: 7282-5548-30
- Service: 88953303
- Description: 2-Way M YESC Weather Pack (BK)

#### Terminal Part Information

- Terminal/Tray: 7116-4102-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: 7114-4103-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-3 (GY)

#### X102 Body Harness to the Battery Cable Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.5 BK | 50 | Ground | 1 | 0.8 BK | 50 | Ground
2 | -- | -- | Not Used | 2 | -- | -- | Not Used

### X103 Left Front Wheel Speed Sensor Harness to the Body Harness

#### Connector Part Information

- OEM: 12052641
- Service: 12102747
- Description: 2-Way F Metri-Pack 150 Series (BK)

#### Connector Part Information

- OEM: 12162000
- Service: 12167120
- Description: 2-Way M Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12048074/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: 12045773/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-3 (GY)

#### X103 Left Front Wheel Speed Sensor Harness to the Body Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.8 YE | 873 | Low Reference | A | 0.5 YE | 873 | Low Reference
B | 0.8 L-BU | 830 | Left Front Wheel Speed Sensor Signal | B | 0.5 L-BU | 830 | Left Front Wheel Speed Sensor Signal

### X104 Right Front Wheel Speed Sensor Harness to the Body Harness

#### Connector Part Information

- OEM: 12052641
- Service: 12102747
- Description: 2-Way F Metri-Pack 150 Series (BK)

#### Connector Part Information

- OEM: 12162000
- Service: 12167120
- Description: 2-Way M Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12048074/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: 12045773/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-3 (GY)

#### X104 Right Front Wheel Speed Sensor Harness to the Body Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.8 TN | 833 | Low Reference | A | 0.5 TN | 833 | Low Reference
B | 0.8 D-GN | 872 | Right Front Wheel Speed Sensor Signal | B | 0.5 D-GN | 872 | Right Front Wheel Speed Sensor Signal

### X105 Engine Harness to the Fuel Injector Harness

#### Connector Part Information

- OEM: 1-967189-1
- Service: See Catalog
- Description: 10-Way F Timer Junior Power Timer Sealed (BK)

#### Connector Part Information

- OEM: 1-962352-1
- Service: See Catalog
- Description: 10-Way M Junior Power Timer Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 4-964286-1/16
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12093647/J-35616-4A (PU)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X105 Engine Harness to the Fuel Injector Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 1.0 PK/BK | 5291 | Ignition Voltage | 1 | 1.0 WH | 5291 | Ignition Voltage
2 | 1.0 PK/BK | 5292 | Ignition Voltage | 2 | 1.0 WH | 5292 | Ignition Voltage
3 | 0.8 TN | 1744 | Fuel Injector 1 Control | 3 | 0.8 TN | 1744 | Fuel Injector 1 Control
4 | 0.8 PK/BK | 1746 | Fuel Injector 3 Control | 4 | 0.8 PK/BK | 1746 | Fuel Injector 3 Control
5 | 0.8 TN/WH | 845 | Fuel Injector 5 Control | 5 | 0.8 TN/WH | 845 | Fuel Injector 5 Control
6 | 0.8 L-GN/BK | 1745 | Fuel Injector 2 Control | 6 | 0.8 L-GN/BK | 1745 | Fuel Injector 2 Control
7 | 0.8 L-BU/BK | 844 | Fuel Injector 4 Control | 7 | 0.8 L-BU/BK | 844 | Fuel Injector 4 Control
8 | 0.8 YE/BK | 846 | Fuel Injector 6 Control | 8 | 0.8 YE/BK | 846 | Fuel Injector 6 Control
9-10 | -- | -- | Not Used | 9-10 | -- | -- | Not Used

### X106 Body Harness to the Engine Harness

#### Connector Part Information

- OEM: 7283-5546-30
- Service: See Catalog
- Description: 12-Way F 1.5 Series Sealed (BK)

#### Connector Part Information

- OEM: 7282-5545-30
- Service: See Catalog
- Description: 12-Way M 1.5 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 7116-4102-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: 7114-4102-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-3 (GY)

#### X106 Body Harness to the Engine Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.35 PU | 1589 | Fuel Level Sensor Signal | 1 | 0.5 PU | 1589 | Fuel Level Sensor Signal
2 | 0.35 PU | 1272 | Low Reference | 2 | 0.5 PU | 1272 | Low Reference
3 | 0.35 L-BU | 1162 | Accelerator Pedal Position Sensor 2 Signal | 3 | 0.5 L-BU | 1162 | Accelerator Pedal Position Sensor 2 Signal
4 | 0.35 WH/BK | 1164 | 5-Volt Reference | 4 | 0.5 WH/BK | 1164 | 5-Volt Reference
5 | 0.35 BN | 1271 | Low Reference | 5 | 0.5 BN | 1271 | Low Reference
6 | 0.5 D-GN | 890 | Fuel Tank Pressure Sensor Signal | 6 | 0.5 D-GN | 890 | Fuel Tank Pressure Sensor Signal
7 | 0.5 GY | 2709 | 5-Volt Reference | 7 | 0.5 GY | 2709 | 5-Volt Reference
8 | 0.35 D-BU | 1161 | Accelerator Pedal Position Sensor 1 Signal | 8 | 0.5 D-BU | 1161 | Accelerator Pedal Position Sensor 1 Signal
9 | 0.35 TN | 1274 | 5-Volt Reference | 9 | 0.5 TN | 1274 | 5-Volt Reference
10 | -- | -- | Not Used | 10 | -- | -- | Not Used
11 | 0.5 TN/BK | 2500 | High Speed GMLAN Serial Data Bus+ | 11 | 0.5 TN/BK | 2500 | High Speed GMLAN Serial Data Bus+
12 | 0.5 TN | 2501 | High Speed GMLAN Serial Data Bus- | 12 | 0.5 TN | 2501 | High Speed GMLAN Serial Data Bus-

### X108 Forward Lamp Harness to the Right Cooling Fan Harness

#### Connector Part Information

- OEM: 7283-5596-10
- Service: 88953307
- Description: 2-Way F YESC/USCAR Class III (D-GY)

#### Connector Part Information

- OEM: 7282-5596-10
- Service: 88953304
- Description: 2-Way M 250 Sealed (D-GY)

#### Terminal Part Information

- Terminal/Tray: 7116-4142-02/10
- Core/Insulation Crimp: A/3
- Release Tool/Test Probe: 12094430/J-35616-42 (RD)

#### Terminal Part Information

- Terminal/Tray: 7114-4142-02/10
- Core/Insulation Crimp: A/3
- Release Tool/Test Probe: 12094430/J-35616-43 (RD)

#### X108 Forward Lamp Harness to the Right Cooling Fan Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 3.0 L-BU | 409 | Cooling Fan Motor Control | 1 | 3.0 L-BU | 409 | Cooling Fan Motor Control
2 | 3.0 BK | 1250 | Ground | 2 | 3.0 BK | 1250 | Ground

### X109 Forward Lamp Harness to the Left Headlamp Harness

#### Connector Part Information

- OEM: 15326822
- Service: 19151498
- Description: 5-Way F GT 150 Sealed 4.0 (BK)

#### Connector Part Information

- OEM: 15326827
- Service: 89046648
- Description: 5-Way M GT 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X109 Forward Lamp Harness to the Left Headlamp Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.35 BK | 1250 | Ground | A | 0.35 BK | 1250 | Ground
B | 0.5 D-GN/WH | 711 | Left Headlamp High Beam Control | B | 0.5 WH | 711 | Left Headlamp High Beam Control
C | 0.5 YE | 712 | Left Headlamp Low Beam Control | C | 0.5 D-GN | 712 | Left Headlamp Low Beam Control
D | 0.35 L-BU/WH | 1314 | Left Front Turn Signal Lamp Control | D | 0.35 D-BU | 1314 | Left Front Turn Signal Lamp Control
E | 0.35 PU | 709 | Left Park Lamp Control | E | 0.35 L-GN | 709 | Left Park Lamp Control

### X110 Forward Lamp Harness to the Right Headlamp Harness

#### Connector Part Information

- OEM: 15326822
- Service: 19151498
- Description: 5-Way F GT 150 Sealed 4.0 (BK)

#### Connector Part Information

- OEM: 15326827
- Service: 89046648
- Description: 5-Way M GT 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X110 Forward Lamp Harness to the Right Headlamp Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.35 BK | 1250 | Ground | A | 0.35 BK | 1250 | Ground
B | 0.5 L-GN/BK | 311 | Right Headlamp High Beam Control | B | 0.5 WH | 311 | Right Headlamp High Beam Control
C | 0.5 TN/WH | 312 | Right Headlamp Low Beam Control | C | 0.5 D-GN | 312 | Right Headlamp Low Beam Control
D | 0.35 D-BU/WH | 1315 | Right Front Turn Signal Lamp Control | D | 0.35 D-BU | 1315 | Right Front Turn Signal Lamp Control
E | 0.35 BN/WH | 309 | Right Park Lamp Control | E | 0.35 L-GN | 309 | Right Park Lamp Control

### X202 Console Harness to the Instrument Panel Harness (C69+UUC)

#### Connector Part Information

- OEM: 7283-8391-40
- Service: See Catalog
- Description: 26-Way F YESC LIF Series (L-GY)

#### Connector Part Information

- OEM: 7282-8391-40
- Service: See Catalog
- Description: 26-Way M YESC LIF Series (L-GY)

#### Terminal Part Information

- Terminal/Tray: 7116-4100-08/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: 7114-4100-08/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

#### X202 Console Harness to the Instrument Panel Harness (C69+UUC)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | -- | -- | Not Used | 1 | -- | -- | Not Used
2 | 0.35 GY | 8 | Instrument Panel Lamp Control | 2 | 0.35 GY | 8 | Instrument Panel Lamp Control
3 | 0.5 BARE | 5346 | Video Drain Wire | 3 | 0.35 BARE | 5346 | Video Drain Wire
4 | 0.5 PU | 2056 | Auxiliary Video High Signal | 4 | 0.5 PU | 2056 | Auxiliary Video High Signal
5 | 0.5 WH | 2058 | Auxiliary Audio Right Signal | 5 | 0.5 WH | 2058 | Auxiliary Audio Right Signal
6 | 0.5 YE | 2059 | Auxiliary Audio Left Signal | 6 | 0.5 YE | 2059 | Auxiliary Audio Left Signal
7 | 0.5 BARE | 5345 | Drain Wire | 7 | 0.35 BARE | 5345 | Drain Wire
8-9 | -- | -- | Not Used | 8-9 | -- | -- | Not Used
10 | 0.35 OG | 2615 | Auxiliary Mode Door Control | 10 | 0.35 OG | 2615 | Auxiliary Mode Door Control
11 | 0.35 GY | 720 | Low Reference | 11 | 0.35 GY/BK | 1798 | Low Reference
0.35 GY | 720 | Low Reference
12 | 0.35 GY | 597 | 5-Volt Reference | 12 | 0.35 GY | 596 | 5-Volt Reference
0.35 GY | 597 | 5-Volt Reference
13 | 0.35 YE | 2214 | Auxiliary Air Temperature Door Control | 13 | 0.35 YE | 2214 | Auxiliary Air Temperature Door Control
14 | 0.35 BK/WH | 1551 | Ground | 14 | 0.35 BK/WH | 1551 | Ground
15 | 0.35 PU/WH | 760 | Auxiliary Blower Motor Speed Control | 15 | 0.35 PU/WH | 760 | Auxiliary Blower Motor Speed Control
16-26 | -- | -- | Not Used | 16-26 | -- | -- | Not Used

### X203 Console Harness to the Instrument Panel Harness (C69-UUC)

#### Connector Part Information

- OEM: 7283-3441-40
- Service: See Catalog
- Description: 8-Way F 1.5 Unsealed (L-GY)

#### Connector Part Information

- OEM: 7282-3441-40
- Service: See Catalog
- Description: 8-Way M 1.5 Unsealed (L-GY)

#### Terminal Part Information

- Terminal/Tray: 7116-4100-08/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: 7114-4100-08/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

#### X203 Console Harness to the Instrument Panel Harness (C69-UUC)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.35 GY | 8 | Instrument Panel Lamp Control | 1 | 0.35 GY | 8 | Instrument Panel Lamp Control
2 | 0.35 BK/WH | 1551 | Ground | 2 | 0.35 BK/WH | 1551 | Ground
3 | 0.35 OG | 2615 | Auxiliary Mode Door Control | 3 | 0.35 OG | 2615 | Auxiliary Mode Door Control
4 | 0.35 GY | 720 | Low Reference | 4 | 0.35 GY/BK | 1798 | Low Reference
0.35 GY | 720 | Low Reference
5 | -- | -- | Not Used | 5 | -- | -- | Not Used
6 | 0.35 GY | 597 | 5-Volt Reference | 6 | 0.35 GY | 597 | 5-Volt Reference
7 | 0.35 YE | 2214 | Auxiliary Air Temperature Door Control | 7 | 0.35 YE | 2214 | Auxiliary Air Temperature Door Control
8 | 0.35 PU/WH | 760 | Auxiliary Blower Motor Speed Control | 8 | 0.35 PU/WH | 760 | Auxiliary Blower Motor Speed Control

### X204 Instrument Panel Harness to the Body Harness

#### Connector Part Information

- OEM: 15336479
- Service: 15306186
- Description: 4-Way F Metri-Pack 280 (YE)

#### Connector Part Information

- OEM: 15336476
- Service: 88987998
- Description: 4-Way M Metri-Pack 280 Series (YE)

#### Terminal Part Information

- Terminal/Tray: 12034046/2
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

#### Terminal Part Information

- Terminal/Tray: 12034047/2
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 12094430/J-35616-5 (PU)

#### X204 Instrument Panel Harness to the Body Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A1 | 0.35 TN | 3021 | Steering Wheel Module - Stage 1 - High Control | A1 | 0.35 TN | 3021 | Steering Wheel Module - Stage 1 - High Control
A2 | 0.35 BN | 3020 | Steering Wheel Module - Stage 1 - Low Control | A2 | 0.35 BN | 3020 | Steering Wheel Module - Stage 1 - Low Control
B1 | 0.35 WH | 3023 | Steering Wheel Module - Stage 2 - High Control | B1 | 0.35 WH | 3023 | Steering Wheel Module - Stage 2 - High Control
B2 | 0.35 PK | 3022 | Steering Wheel Module - Stage 2 - Low Control | B2 | 0.35 PK | 3022 | Steering Wheel Module - Stage 2 - Low Control

### X206 Instrument Panel Harness to the Body Harness

#### Connector Part Information

- OEM: 7283-8391-40
- Service: See Catalog
- Description: 26-Way F YESC LIF Series (L-GY)

#### Connector Part Information

- OEM: 7282-8391-40
- Service: See Catalog
- Description: 26-Way M YESC LIF Series (L-GY)

#### Terminal Part Information

- Pins: 3, 4-6, 13-16, 18-19, 21-25
- Terminal/Tray: 7116-4100-08/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

- Pins: 9-16
- Terminal/Tray: 7116-4101-08/9
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

- Pins: 26
- Terminal/Tray: 7116-4110-02/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

#### Terminal Part Information

- Pins: 3, 4-6, 13-16, 18-19, 21-25
- Terminal/Tray: 7114-4100-08/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

- Pins: 11-16
- Terminal/Tray: 7114-4101-08/9
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

- Pins: 26
- Terminal/Tray: 7114-4110-02/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094430/J-35616-5 (PU)

#### X206 Instrument Panel Harness to the Body Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1-2 | -- | -- | Not Used | 1-2 | -- | -- | Not Used
3 | 0.5 TN/BK | 2500 | High Speed GMLAN Serial Data Bus+ | 3 | 0.5 TN/BK | 2500 | High Speed GMLAN Serial Data Bus+
4 | 0.5 TN | 2501 | High Speed GMLAN Serial Data Bus- | 4 | 0.5 TN | 2501 | High Speed GMLAN Serial Data Bus-
5 | -- | -- | Not Used | 5 | -- | -- | Not Used
6 | 0.5 OG | 5748 | Radio Audio Mute Signal (U65) | 6 | 0.5 OG | 5748 | Radio Audio Mute Signal (U65)
7-8 | -- | -- | Not Used | 7-8 | -- | -- | Not Used
9 | 0.75 TN | 1875 | Right Front Speaker Output (+) | 9 | 0.5 L-GN/WH | 512 | Right Front Low Level Audio Signal (+) (U65)
0.8 L-GN | 200 | Right Front Speaker Output (+) (-U65)
10 | 0.75 TN/WH | 1975 | Right Front Speaker Output (-) | 10 | 0.5 L-GN | 1948 | Right Front Low Level Audio Signal (-) (U65)
0.8 D-GN | 117 | Right Front Speaker Output (-) (-U65)
11 | 0.75 GY | 118 | Left Front Speaker Output (-) | 11 | 0.5 D-GN | 1947 | Left Front Low Level Audio Signal (-) (U65)
0.8 GY | 118 | Left Front Speaker Output (-) (-U65)
12 | 0.75 TN | 201 | Left Front Speaker Output (+) | 12 | 0.5 TN | 511 | Left Front Low Level Audio Signal (+) (U65)
0.8 TN | 201 | Left Front Speaker Output (+) (-U65)
13 | 0.75 BN | 199 | Left Rear Speaker Output (+) | 13 | 0.5 BN/WH | 599 | Left Rear Low Level Audio Signal (+) (U65)
0.8 BN | 199 | Left Rear Speaker Output (+) (-U65)
14 | 0.75 YE | 116 | Left Rear Low Level Audio Signal (-) | 14 | 0.8 YE | 116 | Left Rear Speaker Output (-) (-U65)
0.5 BN | 1999 | Left Rear Low Level Audio Signal (-) (U65)
15 | 0.75 L-BU | 115 | Right Rear Speaker Output (-) | 15 | 0.8 L-BU | 115 | Right Rear Speaker Output (-) (-U65)
0.5 TN | 1946 | Right Rear Low Level Audio Signal (-) (U65)
16 | 0.75 D-BU | 46 | Right Rear Speaker Output (+) | 16 | 0.5 D-BU | 546 | Right Rear Low Level Audio Signal (+) (U65)
0.8 D-BU | 46 | Right Rear Speaker Output (+) (-U65)
17 | -- | -- | Not Used | 17 | -- | -- | Not Used
18 | 0.35 BARE | 1489 | Drain Wire (U3U) | 18 | 0.35 BARE | 1489 | Drain Wire (U3U)
19 | 0.5 GY | 655 | Cellular Microphone Signal (U3U) | 19 | 0.5 GY | 655 | Cellular Microphone Signal (U3U)
20 | -- | -- | Not Used | 20 | -- | -- | Not Used
21 | 0.5 TN/WH | 372 | Remote Radio Audio Output (-) (U2K) | 21 | 0.5 TN/WH | 372 | Remote Radio Audio Output (-) (U2K)
22 | 0.5 BN/WH | 367 | Remote Radio Left Audio Signal (U2K) | 22 | 0.5 BN/WH | 367 | Remote Radio Left Audio Signal (U2K)
23 | 0.5 GY | 388 | Remote Radio Right Audio Signal (U2K) | 23 | 0.5 GY | 388 | Remote Radio Right Audio Signal (U2K)
24 | 0.5 D-GN/WH | 368 | Remote Radio Right Audio Signal (U2K) | 24 | 0.5 D-GN/WH | 368 | Remote Radio Right Audio Signal (U2K)
25 | 0.35 BARE | 6759 | Discrete Audio Drain Wire (U2K) | 25 | 0.35 BARE | 6759 | Discrete Audio Drain Wire (U2K)
26 | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data | 26 | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data

### X207 Console Harness to the Instrument Panel Harness (UUC-C69)

#### Connector Part Information

- OEM: 7283-6387-40
- Service: See Catalog
- Description: 6-Way F (L-GY)

#### Connector Part Information

- OEM: 7282-6561-40
- Service: See Catalog
- Description: 6-Way M Unsealed (L-GY)

#### Terminal Part Information

- Terminal/Tray: 7116-4720-02/14
- Core/Insulation Crimp: Pins: 6 : H/H
- Core/Insulation Crimp: Pins: 1-5 : J/J
- Release Tool/Test Probe: 15315247/J-35616-64B (L-BU)

#### Terminal Part Information

- Terminal/Tray: 7114-4721-02/14
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: 15315247/J-35616-65B (L-BU)

#### X207 Console Harness to the Instrument Panel Harness (UUC-C69)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.5 BARE | 5346 | Video Drain Wire | 1 | 0.35 BARE | 5346 | Video Drain Wire
2 | 0.5 PU | 2056 | Auxiliary Video High Signal | 2 | 0.5 PU | 2056 | Auxiliary Video High Signal
3 | 0.5 WH | 2058 | Auxiliary Audio Right Signal | 3 | 0.5 WH | 2058 | Auxiliary Audio Right Signal
4 | 0.5 YE | 2059 | Auxiliary Audio Left Signal | 4 | 0.5 YE | 2059 | Auxiliary Audio Left Signal
5 | 0.5 BARE | 5345 | Drain Wire | 5 | 0.35 BARE | 5345 | Drain Wire
6 | -- | -- | Not Used | 6 | -- | -- | Not Used

### X210 Instrument Panel Harness to the Body Harness

#### Connector Part Information

- OEM: 7283-8391-40
- Service: See Catalog
- Description: 26-Way F YESC LIF Series (L-GY)

#### Connector Part Information

- OEM: 7282-8391-40
- Service: See Catalog
- Description: 26-Way M YESC LIF Series (L-GY)

#### Terminal Part Information

- Pins: 1
- Terminal/Tray: 7116-4121-02/10
- Core/Insulation Crimp: C/B
- Release Tool/Test Probe: 12094430/J-35616-42 (RD)

- Pins: 2-7, 5, 9-16, 18-25
- Terminal/Tray: 7116-4100-08/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

- Pins: 8
- Terminal/Tray: 7116-4120-02/9
- Core/Insulation Crimp: E/B
- Release Tool/Test Probe: 12094430/J-35616-42 (RD)

- Pins: 26, 17
- Terminal/Tray: 7116-4110-02/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

#### Terminal Part Information

- Pins: 1
- Terminal/Tray: 7114-4121-02/9
- Core/Insulation Crimp: C/B
- Release Tool/Test Probe: 12094430/J-35616-43 (RD)

- Pins: 2-7, 5, 9-16, 18-25
- Terminal/Tray: 7114-4100-08/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

- Pins: 8
- Terminal/Tray: 7114-4120-02/9
- Core/Insulation Crimp: E/B
- Release Tool/Test Probe: 12094430/J-35616-43 (RD)

- Pins: 26, 17
- Terminal/Tray: 7114-4110-02/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094430/J-35616-5 (PU)

#### X210 Instrument Panel Harness to the Body Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | -- | -- | Not Used | 1 | -- | -- | Not Used
2 | 0.5 WH/BK | 6436 | CAN Bus Low Terminated Serial Data | 2 | 0.5 WH/BK | 6436 | CAN Bus Low Terminated Serial Data
3 | 0.5 BN/WH | 6437 | CAN Bus High Terminated Serial Data | 3 | 0.5 BN/WH | 6437 | CAN Bus High Terminated Serial Data
4 | 0.5 OG/BK | 6045 | Low Reference | 4 | 0.5 OG/BK | 6045 | Low Reference
5 | 0.5 GY | 6044 | 5-Volt Reference | 5 | 0.5 GY | 6044 | 5-Volt Reference
6 | 0.5 TN/WH | 6433 | CAN Bus High Serial Data | 6 | 0.5 TN/WH | 6433 | CAN Bus High Serial Data
7 | 0.5 L-GN/BK | 6432 | CAN Bus Low Serial Data | 7 | 0.5 L-GN/BK | 6432 | CAN Bus Low Serial Data
8 | 1.0 RD/WH | 2540 | Battery Positive Voltage | 8 | 1.0 RD/WH | 2540 | Battery Positive Voltage
9 | 0.35 L-GN/BK | 735 | Ambient Air Temperature Sensor Signal | 9 | 0.35 L-GN/BK | 735 | Ambient Air Temperature Sensor Signal
10 | 0.35 YE | 61 | Low Reference | 10 | 0.35 YE | 61 | Low Reference
11 | 0.5 TN/BK | 2500 | High Speed GMLAN Serial Data Bus+ | 11 | 0.5 TN/BK | 2500 | High Speed GMLAN Serial Data Bus+
0.5 TN/BK | 2500 | High Speed GMLAN Serial Data Bus+
12 | 0.5 TN | 2501 | High Speed GMLAN Serial Data Bus- | 12 | 0.5 TN | 2501 | High Speed GMLAN Serial Data Bus-
0.5 TN | 2501 | High Speed GMLAN Serial Data Bus-
13 | 0.5 BN/WH | 419 | Malfunction Indicator Lamps Control | 13 | 0.5 BN/WH | 419 | Malfunction Indicator Lamps Control
14 | 0.35 L-GN | 1499 | Driver Mirror Motor Left/Down Control | 14 | 0.35 L-GN | 1499 | Driver Mirror Motor Left/Down Control
15 | 0.35 PU/WH | 889 | Passenger Mirror Motor Down Control | 15 | 0.35 PU/WH | 889 | Passenger Mirror Motor Down Control
16 | 0.35 OG/WH | 881 | Passenger Mirror Motor Right Control | 16 | 0.35 OG/WH | 881 | Passenger Mirror Motor Right Control
17 | 0.5 D-GN/WH | 817 | Vehicle Speed Signal (U3U) | 17 | 0.5 D-GN/WH | 817 | Vehicle Speed Signal (U3U)
18 | 0.35 BN | 1271 | Low Reference | 18 | 0.35 BN | 1271 | Low Reference
19 | 0.35 D-BU | 1161 | Accelerator Pedal Position Sensor 1 Signal | 19 | 0.35 D-BU | 1161 | Accelerator Pedal Position Sensor 1 Signal
20 | 0.35 WH/BK | 1164 | 5-Volt Reference | 20 | 0.35 WH/BK | 1164 | 5-Volt Reference
21 | 0.35 TN | 1274 | 5-Volt Reference | 21 | 0.35 TN | 1274 | 5-Volt Reference
22 | 0.35 L-BU | 1162 | Accelerator Pedal Position Sensor 2 Signal | 22 | 0.35 L-BU | 1162 | Accelerator Pedal Position Sensor 2 Signal
23 | 0.35 PU | 1272 | Low Reference | 23 | 0.35 PU | 1272 | Low Reference
24 | 0.35 TN/WH | 33 | Brake Warning Indicator Control | 24 | 0.35 TN/WH | 33 | Brake Warning Indicator Control
25 | 0.35 YE | 88 | Driver Mirror Motor Up Control | 25 | 0.35 YE | 88 | Driver Mirror Motor Up Control
26 | 0.35 WH | 81 | Driver Mirror Motor Right Control | 26 | 0.35 WH | 81 | Driver Mirror Motor Right Control

### X214 Passenger Airbag Jumper Harness to the Instrument Panel Harness

#### Connector Part Information

- OEM: 15336479
- Service: 15306186
- Description: 4-Way F Metri-Pack 280 Series (YE)

#### Connector Part Information

- OEM: 15336476
- Service: 88987998
- Description: 4-Way M Metri-Pack 280 Series (YE)

#### Terminal Part Information

- Terminal/Tray: Service With Pigtail
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Terminal/Tray: Service With Pigtail
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: 12094430/J-35616-5 (PU)

#### X214 Passenger Airbag Jumper Harness to the Instrument Panel Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A1 | 0.35 YE | 3025 | Instrument Panel Module - Stage 1 - High Control | A1 | 0.35 YE | 3025 | Instrument Panel Module - Stage 1 - High Control
A2 | 0.35 OG | 3024 | Instrument Panel Module - Stage 1 - Low Control | A2 | 0.35 OG | 3024 | Instrument Panel Module - Stage 1 - Low Control
B1 | 0.35 GY | 3027 | Instrument Panel Module - Stage 2 - High Control | B1 | 0.35 GY | 3027 | Instrument Panel Module - Stage 2 - High Control
B2 | 0.35 PU | 3026 | Instrument Panel Module - Stage 2 - Low Control | B2 | 0.35 PU | 3026 | Instrument Panel Module - Stage 2 - Low Control

### X216 Instrument Panel Harness to the HVAC Harness

#### Connector Part Information

- OEM: 15332177
- Service: See Catalog
- Description: 16-Way F GT 150 (BK)

#### Connector Part Information

- OEM: 15332182
- Service: 15306371
- Description: 16-Way M GT 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12191812/19
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X216 Instrument Panel Harness to the HVAC Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.35 WH | 119 | Mode Door Control | A | 0.35 WH | 119 | Mode Door Control
B | 0.35 TN/BK | 2274 | Recirculation Door Control Circuit | B | 0.35 TN/BK | 2274 | Recirculation Door Control Circuit
C | 0.35 TN | 2273 | Mode Door Control | C | 0.35 TN | 2273 | Mode Door Control
D | 0.35 TN | 516 | Upper Left Air Temperature Sensor Signal | D | 0.35 TN | 516 | Upper Left Air Temperature Sensor Signal
E | 0.35 TN | 520 | Lower Right Air Temperature Sensor Signal | E | 0.35 TN | 520 | Lower Right Air Temperature Sensor Signal
F | 0.35 YE | 1791 | Low Reference | F | 0.35 YE | 1791 | Low Reference
G | 0.35 PU | 1838 | Recirculation Door Position Signal | G | 0.35 PU | 1838 | Recirculation Door Position Signal
H | 0.35 L-BU | 733 | Air Temperature Door Position Signal | H | 0.35 L-BU | 733 | Air Temperature Door Position Signal
J | 0.35 L-GN | 2275 | Mode Door Position Signal | J | 0.35 L-GN | 2275 | Mode Door Position Signal
K | 0.35 D-GN | 1614 | Recirculation Door Control | K | 0.35 D-GN | 1614 | Recirculation Door Control
L | 0.35 D-BU | 1199 | Air Temperature Door Control | L | 0.35 D-BU | 1199 | Air Temperature Door Control
M | 0.35 L-BU | 1316 | Air Temperature Door Control | M | 0.35 L-BU | 1316 | Air Temperature Door Control
N | 0.35 GY | 598 | 5-Volt Reference | N | 0.35 GY | 598 | 5-Volt Reference
P | 0.35 WH | 2622 | 5-Volt Reference | P | 0.35 WH | 2622 | 5-Volt Reference
R | 0.35 TN | 552 | Low Reference | R | 0.35 TN | 552 | Low Reference
S | 0.35 YE | 61 | Low Reference | S | 0.35 YE | 61 | Low Reference

### X218 Instrument Panel Harness to the Body Harness

#### Connector Part Information

- OEM: 15336479
- Service: 15306186
- Description: 4-Way F Metri-Pack 280 (YE)

#### Connector Part Information

- OEM: 15336476
- Service: See Catalog
- Description: 4-Way M Metri-Pack 280 (YE)

#### Terminal Part Information

- Terminal/Tray: 12034046/2
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X218 Instrument Panel Harness to the Body Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A1 | 0.35 YE | 3025 | Instrument Panel Module - Stage 1 - High Control | A1 | 0.35 YE | 3025 | Instrument Panel Module - Stage 1 - High Control
A2 | 0.35 OG | 3024 | Instrument Panel Module - Stage 1 - Low Control | A2 | 0.35 OG | 3024 | Instrument Panel Module - Stage 1 - Low Control
B1 | 0.35 GY | 3027 | Instrument Panel Module - Stage 2 - High Control | B1 | 0.35 GY | 3027 | Instrument Panel Module - Stage 2 - High Control
B2 | 0.35 PU | 3026 | Instrument Panel Module - Stage 2 - Low Control | B2 | 0.35 PU | 3026 | Instrument Panel Module - Stage 2 - Low Control

### X219 Body Harness to the Instrument Panel Harness

#### Connector Part Information

- OEM: GT13GM-1/1S-HU
- Service: See Catalog
- Description: 3-Way F GT13 Coaxial Series (GY)

#### Connector Part Information

- OEM: GT13GM-1/1PPHU
- Service: See Catalog
- Description: 3-Way M GT13 Coaxial Series (GY)

#### Terminal Part Information

- Terminal/Tray: 7116-4618-02/14
- Core/Insulation Crimp: P/P
- Release Tool/Test Probe: J-38125-215/J-35616-64B (L-BU)

#### Terminal Part Information

- Terminal/Tray: 7114-4618-02/27
- Core/Insulation Crimp: P/P
- Release Tool/Test Probe: J-38125-215/J-35616-65B (L-BU)

#### X219 Body Harness to the Instrument Panel Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.5 WH | 1487 | Antenna Enable Signal | 1 | 0.5 WH | 1487 | Antenna Enable Signal
C | COAX | 6001 | Antenna RF Signal | C | COAX | 6001 | Antenna RF Signal
S | COAX | 6015 | Shield | S | COAX | 6015 | Shield

### X223 Sunload/Ambient Light Sensor Harness to the Instrument Panel Harness

#### Connector Part Information

- OEM: 7283-6446-40
- Service: See Catalog
- Description: 4-Way F Kaizen YESC Series (GY)

#### Connector Part Information

- OEM: 7282-6446-40
- Service: See Catalog
- Description: 4-Way M Kaizen YESC Series (GY)

#### Terminal Part Information

- Terminal/Tray: 7116-4110-02/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

#### Terminal Part Information

- Pins: 1-2, 4
- Terminal/Tray: 7114-4110-02/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094430/J-35616-5 (PU)

- Pins: 3
- Terminal/Tray: 7114-4111-02/9
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 12094430/J-35616-5 (PU)

#### X223 Sunload/Ambient Light Sensor Harness to the Instrument Panel Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.35 GY | 1548 | Passenger Sunload Sensor Signal | 1 | 0.35 GY | 1548 | Passenger Sunload Sensor Signal
2 | 0.35 L-BU/BK | 590 | Driver Sunload Sensor Signal | 2 | 0.35 L-BU/BK | 590 | Driver Sunload Sensor Signal
3 | 0.35 L-GN/BK | 1137 | Daytime Running Lamp Ambient Light Sensor Signal | 3 | 0.35 L-GN/BK | 1137 | Daytime Running Lamp Ambient Light Sensor Signal
4 | 0.35 BK/WH | 1551 | Ground | 4 | 0.35 BK/WH | 1551 | Ground

### X226 Instrument Panel Harness to the Shifter Jumper Harness

#### Connector Part Information

- OEM: 936268-1
- Service: See Catalog
- Description: 6-Way F 090 Series (WH)

#### Connector Part Information

- OEM: 936271-1
- Service: See Catalog
- Description: 6-Way M 090 Series (WH)

#### Terminal Part Information

- Terminal/Tray: 368083-1/26
- Core/Insulation Crimp: E/2
- Release Tool/Test Probe: 15315247/J-35616-18 (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X226 Instrument Panel Harness to the Shifter Jumper Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.35 PU | 1375 | 12-Volt Reference | 1 | 0.35 PU | 1375 | 12-Volt Reference
0.35 PU | 1375 | 12-Volt Reference
2 | 0.35 PU/WH | 5905 | Key Capture/Column Lock Shift Position Signal | 2 | 0.35 GY | 5905 | Key Capture/Column Lock Shift Position Signal
3 | .35 BK | 1450 | Ground | 3 | 1.0 BK | 1450 | Ground
4 | 0.35 PU | 5526 | Tap Up/Tap Down Switch Signal | 4 | 0.35 BK | 5526 | Tap Up/Tap Down Switch Signal
5 | 0.35 PU/WH | 1630 | Steering Column Key Cylinder Lock Solenoid Control | 5 | 0.35 BN | 1630 | Steering Column Key Cylinder Lock Solenoid Control
6 | 0.35 D-GN/WH | 1135 | Automatic Transmission Shift Lock Control Solenoid Control | 6 | 0.35 D-GN/WH | 1135 | Automatic Transmission Shift Lock Control Solenoid Control

### X275 Instrument Panel Harness to the Steering Wheel Module Coil Harness

#### Connector Part Information

- OEM: 15393421
- Service: 88987853
- Description: 4-Way F Micro-Pack 064 Series (YE)

#### Connector Part Information

- OEM: 15393425
- Service: See Catalog
- Description: 4-Way M Micro-Pack 064 Series (YE)

#### Terminal Part Information

- Terminal/Tray: Service With Pigtail
- Core/Insulation Crimp: E/2
- Release Tool/Test Probe: 12180559-1/J-35616-64B (L-BU)

#### Terminal Part Information

- Terminal/Tray: Service With Pigtail
- Core/Insulation Crimp: Service With Pigtail
- Release Tool/Test Probe: Service With Pigtail

#### X275 Instrument Panel Harness to the Steering Wheel Module Coil Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.35 BN | 3020 | Steering Wheel Module - Stage 1 - Low Control | 1 | -- | 3020 | Steering Wheel Module - Stage 1 - Low Control
2 | 0.35 TN | 3021 | Steering Wheel Module - Stage 1 - High Control | 2 | -- | 3021 | Steering Wheel Module - Stage 1 - High Control
3 | 0.35 PK | 3022 | Steering Wheel Module - Stage 2 - Low Control | 3 | -- | 3022 | Steering Wheel Module - Stage 2 - Low Control
4 | 0.35 WH | 3023 | Steering Wheel Module - Stage 2 - High Control | 4 | -- | 3023 | Steering Wheel Module - Stage 2 - High Control

### X276 Instrument Panel Harness to the Steering Wheel Module Coil Harness

#### Connector Part Information

- OEM: 15393433
- Service: See Catalog
- Description: 10-Way F Micro-Pack 064 Series (BK)

#### Connector Part Information

- OEM: 15393436
- Service: See Catalog
- Description: 10-Way M Micro-Pack 064 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12177007/19
- Core/Insulation Crimp: E/2
- Release Tool/Test Probe: 12180559-1/J-35616-64B (L-BU)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X276 Instrument Panel Harness to the Steering Wheel Module Coil Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A-B | -- | -- | Not Used | A-B | -- | -- | Not Used
C | 0.35 PU | 1375 | 12-Volt Reference | C | -- | 1375 | 12-Volt Reference
D | 0.35 GY | 1884 | Cruise Control Switch Signal | D | -- | 1884 | Cruise Control Switch Signal
E | 0.35 D-BU | 1796 | Steering Wheel Controls Signal (UK3) | E | -- | 1796 | Steering Wheel Controls Signal (UK3)
F | 0.35 GN/WH | 7158 | Cruise Control Indicator Dimming Signal | F | -- | 7158 | Cruise Control Indicator Dimming Signal
G | 0.35 PU/WH | 7005 | LED Dimming Signal | G | -- | 7005 | LED Dimming Signal
H | -- | -- | Not Used | H | -- | -- | Not Used
J | 0.35 TN | 28 | Horn Relay Control | J | -- | 28 | Horn Relay Control
K | 0.35 BK | 1450 | Ground | K | -- | 1450 | Ground

### X277 Steering Wheel Controls Harness to the Steering Wheel Module Coil Harness

#### Connector Part Information

- OEM: 15393433
- Service: See Catalog
- Description: 10-Way F Micro-Pack 064 Series (BK)

#### Connector Part Information

- OEM: 15393436
- Service: See Catalog
- Description: 10-Way M Micro-Pack 064 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 7116-4111-02/9
- Core/Insulation Crimp: C/A
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

#### Terminal Part Information

- Terminal/Tray: 7114-4111-02/9
- Core/Insulation Crimp: C/A
- Release Tool/Test Probe: 12094430/J-35616-5 (PU)

#### X277 Steering Wheel Controls Harness to the Steering Wheel Module Coil Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A-B | -- | -- | Not Used | A-B | -- | -- | Not Used
C | 0.35 PU | 1375 | 12-Volt Reference | C | 0.35 PU | 1375 | 12-Volt Reference
D | 0.35 GY | 1884 | Cruise Control Switch Signal | D | 0.35 GY | 1884 | Cruise Control Switch Signal
E | 0.35 D-BU | 1796 | Steering Wheel Controls Signal (UK3) | E | 0.35 D-BU | 1796 | Steering Wheel Controls Signal (UK3)
F | GN/WH | 7158 | Cruise Control Indicator Dimming Signal | F | GN/WH | 7158 | Cruise Control Indicator Dimming Signal
G | 0.35 PU/WH | 7005 | LED Dimming Signal | G | 0.35 PU/WH | 7005 | LED Dimming Signal
H | -- | -- | Not Used | H | -- | -- | Not Used
J | 0.35 TN | 28 | Horn Relay Control | J | 0.35 TN | 28 | Horn Relay Control
K | 0.35 BK | 1450 | Ground | K | 0.35 BK | 1450 | Ground

### X305 Console Harness to the Body Harness

#### Connector Part Information

- OEM: 7283-5565-40
- Service: See Catalog
- Description: 2-Way F 110 Unsealed (L-GY)

#### Connector Part Information

- OEM: 7282-5565-40
- Service: See Catalog
- Description: 2-Way M 110 Unsealed (L-GY)

#### Terminal Part Information

- Terminal/Tray: 7116-4111-02/9
- Core/Insulation Crimp: C/A
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

#### Terminal Part Information

- Terminal/Tray: 7114-4111-02/9
- Core/Insulation Crimp: C/A
- Release Tool/Test Probe: 12094430/J-35616-5 (PU)

#### X305 Console Harness to the Body Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 1.0 BK | 650 | Ground | 1 | 1.0 BK | 650 | Ground
2 | 1.0 RD/WH | 2540 | Battery Positive Voltage | 2 | 1.0 RD/WH | 2540 | Battery Positive Voltage

### X307 Body Harness to the Instrument Panel Harness (C69)

#### Connector Part Information

- OEM: 7283-9088-30
- Service: See Catalog
- Description: 10-Way F Kaizen 0.64 Series (BK)

#### Connector Part Information

- OEM: 7282-9082-30
- Service: See Catalog
- Description: 10-Way M Kaizen 0.64 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 7116-4618-02/14
- Core/Insulation Crimp: P/P
- Release Tool/Test Probe: J-38125-215/J-35616-64B (L-BU)

#### Terminal Part Information

- Terminal/Tray: 7114-4618-02/27
- Core/Insulation Crimp: P/P
- Release Tool/Test Probe: J-38125-215/J-35616-65B (L-BU)

#### X307 Body Harness to the Instrument Panel Harness (C69)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.35 GY/BK | 1798 | Low Reference | 1 | 0.35 GY/BK | 1798 | Low Reference
2 | 0.35 GY | 2599 | Auxiliary Mode Door Control | 2 | 0.35 GY | 2599 | Auxiliary Mode Door Control
3 | 0.35 GY | 596 | 5-Volt Reference | 3 | 0.35 GY | 596 | 5-Volt Reference
4 | 0.35 L-GN/WH | 5729 | Rear Mode Motor Control | 4 | 0.35 L-GN/WH | 5729 | Rear Mode Motor Control
5 | 0.35 OG | 2215 | Auxiliary Mode Door Control | 5 | 0.35 OG | 2215 | Auxiliary Mode Door Control
6 | 0.35 PK | 2145 | Air Temperature Switch Signal - Right | 6 | 0.35 PK | 2145 | Air Temperature Switch Signal - Right
7 | 0.35 BN | 6555 | Rear Temperature Motor Control | 7 | 0.35 BN | 6555 | Rear Temperature Motor Control
8 | 0.35 GY | 2614 | Auxiliary Air Temperature Door Control | 8 | 0.35 GY | 2614 | Auxiliary Air Temperature Door Control
9 | 0.35 GY/BK | 754 | Blower Motor Speed Control | 9 | 0.35 GY/BK | 754 | Blower Motor Speed Control
10 | -- | -- | Not Used | 10 | -- | -- | Not Used

### X308 Body Harness to the Power Seat Harness (AG1 -KA1)

#### Connector Part Information

- OEM: 15326886
- Service: 88988300
- Description: 4-Way F GT 280 (BK)

#### Connector Part Information

- OEM: 15326890
- Service: 88953361
- Description: 4-Way M GT 280 Series (BK)

#### Terminal Part Information

- Pins: A-B
- Terminal/Tray: 15304713/19
- Core/Insulation Crimp: 4/4
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

- Pins: C-D
- Terminal/Tray: 15304711/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X308 Body Harness to the Power Seat Harness (AG1 -KA1)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 2.0 RD/BK | 542 | Battery Positive Voltage | A | 2.0 RD/BK | 542 | Battery Positive Voltage
B | 2.0 BK | 650 | Ground | B | 0.35 BK | 650 | Ground
C | 0.35 PK | 5057 | Low Reference | C | 0.35 TN/WH | 5057 | Low Reference
D | 0.35 D-GN | 5016 | Seat Belt Switch - Left - Signal | D | 0.35 D-BU | 5016 | Seat Belt Switch - Left - Signal

### X308 Body Harness to the Driver Seat Harness (KA1)

#### Connector Part Information

- OEM: 15326924
- Service: 15306174
- Description: 8-Way F GT 280 (BK)

#### Connector Part Information

- OEM: 15326928
- Service: 15306176
- Description: 8-Way M GT 280 Series (BK)

#### Terminal Part Information

- Pins: A, B
- Terminal/Tray: 15304713/19
- Core/Insulation Crimp: 4/4
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

- Pins: C-H
- Terminal/Tray: 15304711/8
- Core/Insulation Crimp: Pins: E, G : 2/A
- Core/Insulation Crimp: Pins: C, D, F, H : E/A
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X308 Body Harness to the Driver Seat Harness (KA1)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 2.0 RD/BK | 542 | Battery Positive Voltage | A | 2.0 RD/BK | 542 | Battery Positive Voltage
B | 2.0 BK | 650 | Ground | B | 2.0 BK | 650 | Ground
C | 0.35 PK | 5057 | Low Reference | C | 0.35 PK | 5057 | Low Reference
D | 0.35 D-GN | 5016 | Seat Belt Switch - Left - Signal | D | 0.35 BK | 5016 | Seat Belt Switch - Left - Signal
E | 0.8 PU | 2424 | Driver Heated Seat Back Element Control | E | 0.8 PU | 2424 | Driver Heated Seat Back Element Control
F | 0.35 YE/BK | 2079 | Heated Seat Cushion Temperature Sensor Signal | F | 0.35 YE/BK | 2079 | Heated Seat Cushion Temperature Sensor Signal
G | 0.8 PK | 2077 | Heated Seat Cushion Element Control | G | 0.8 RD/WH | 2077 | Heated Seat Cushion Element Control
H | 0.35 YE | 2080 | Low Reference | H | 0.35 YE | 2080 | Low Reference

### X309 Body Harness to the Passenger Seat Harness (-KA1)

#### Connector Part Information

- OEM: 15332138
- Service: See Catalog
- Description: 5-Way F GT 150 Series (BK)

#### Connector Part Information

- OEM: 15332139
- Service: See Catalog
- Description: 5-Way M GT 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12191812/19
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X309 Body Harness to the Passenger Seat Harness (-KA1)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.35 RD/WH | 840 | Battery Positive Voltage | A | 0.35 RD/WH | 840 | Battery Positive Voltage
B | 0.35 BK/WH | 651 | Ground | B | 0.35 BK/WH | 651 | Ground
C | 0.35 PK | 5057 | Low Reference | C | 0.35 PK | 5057 | Low Reference
D | 0.35 OG | 1362 | Seat Belt Switch - Right - Signal | D | 0.35 RD | 1362 | Seat Belt Switch - Right - Signal
E | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data | E | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data

### X309 Body Harness to the Passenger Seat Harness (KA1)

#### Connector Part Information

- OEM: 15332161
- Service: 15306416
- Description: 12-Way F GT 150 (BK)

#### Connector Part Information

- OEM: 15332166
- Service: See Catalog
- Description: 12-Way M GT 150 Series (BK)

#### Terminal Part Information

- Pins: A-H, J-L
- Terminal/Tray: 12191812/19
- Core/Insulation Crimp: Pins: G, H, J, L : C/A
- Core/Insulation Crimp: Pins: A-F, K : E/C
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X309 Body Harness to the Passenger Seat Harness (KA1)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.35 RD/WH | 840 | Battery Positive Voltage | A | 0.35 RD/WH | 840 | Battery Positive Voltage
B | 0.35 BK/WH | 651 | Ground | B | 0.35 BK/WH | 651 | Ground
C | 0.35 PK | 5057 | Low Reference | C | 0.35 PK | 5057 | Low Reference
D | 0.35 OG | 1362 | Seat Belt Switch - Right - Signal | D | 0.35 RD | 1362 | Seat Belt Switch - Right - Signal
E | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data | E | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data
F | 0.35 YE/BK | 2079 | Heated Seat Cushion Temperature Sensor Signal | F | 0.35 YE | 2079 | Heated Seat Cushion Temperature Sensor Signal
G | 0.8 PK | 2077 | Heated Seat Cushion Element Control | G | 0.8 RD/WH | 2077 | Heated Seat Cushion Element Control
H | 0.8 PU | 2424 | Driver Heated Seat Back Element Control | H | 0.8 PU | 2424 | Driver Heated Seat Back Element Control
J | 1.0 BK | 650 | Ground | J | 2.0 BK | 650 | Ground
K | 0.35 YE | 2080 | Low Reference | K | 0.35 YE | 2080 | Low Reference
L | 1.0 RD/WH | 640 | Battery Positive Voltage | L | 1.0 OG | 640 | Battery Positive Voltage
M | -- | -- | Not Used | M | -- | -- | Not Used

### X311 Headliner Harness to the Dome Lamp Harness (UUC)

#### Connector Part Information

- OEM: 12045813
- Service: 12101889
- Description: 4-Way F Metri-Pack 150 Series (CM)

#### Connector Part Information

- OEM: 12052054
- Service: 88988619
- Description: 4-Way M Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X311 Headliner Harness to the Dome Lamp Harness (UUC)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.8 D-BU/WH | 149 | Courtesy Lamp Supply Voltage | A | 0.8 D-BU/WH | 149 | Courtesy Lamp Supply Voltage
B | 0.8 GY | 157 | Courtesy Lamp Control | B | 0.8 GY | 157 | Courtesy Lamp Control
C | 0.8 OG | 1732 | Courtesy Lamp Supply Voltage | C | 0.8 OG | 1732 | Courtesy Lamp Supply Voltage
D | 0.8 BK | 850 | Ground | D | 0.8 BK | 850 | Ground

### X312 Driver Seat Harness to the Power Seat Harness (AG1 +KA1)

#### Connector Part Information

- OEM: 15326886
- Service: 88988300
- Description: 4-Way F GT 280 Series (BK)

#### Connector Part Information

- OEM: 15326890
- Service: 88953361
- Description: 4-Way M GT 280 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X312 Driver Seat Harness to the Power Seat Harness (AG1 +KA1)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 2.0 RD/BK | 542 | Battery Positive Voltage | A | 2.0 RD/BK | 542 | Battery Positive Voltage
B | 2.0 BK | 650 | Ground | B | 2.0 BK | 650 | Ground
C | 0.35 PK | 5057 | Low Reference | C | 0.35 PK | 5057 | Low Reference
D | 0.35 BK | 5016 | Seat Belt Switch - Left - Signal | D | 0.35 D-BU | 5016 | Seat Belt Switch - Left - Signal

### X313 Passenger Presence Harness to the Passenger Seat Harness

#### Connector Part Information

- OEM: 15332141
- Service: 88986249
- Description: 6-Way F GT 150 Series (BK)

#### Connector Part Information

- OEM: 15332142
- Service: 89046638
- Description: 6-Way M GT 150/280 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X313 Passenger Presence Harness to the Passenger Seat Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.35 OG | 840 | Battery Positive Voltage | A | 0.35 RD/WH | 840 | Battery Positive Voltage
B | 0.35 YE | 5060 | Low Speed GMLAN Serial Data | B | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data
C | 0.35 WH | 5060 | Low Speed GMLAN Serial Data | C | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data
D | 0.35 BK | 651 | Ground | D | 0.35 BK | 651 | Ground
E-F | -- | -- | Not Used | E-F | -- | -- | Not Used

### X314 Headliner Harness to the Sunroof Harness (CF5)

#### Connector Part Information

- OEM: 12047886
- Service: 12101822
- Description: 8-Way F Metri-Pack 150 Series (BK)

#### Connector Part Information

- OEM: 12045688
- Service: 12101827
- Description: 8-Way M Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X314 Headliner Harness to the Sunroof Harness (CF5)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.35 BN | 100 | Sunroof Switch Open Signal | A | 0.35 BN | 100 | Sunroof Switch Open Signal
B | 0.35 D-GN | 2074 | Sunroof Switch Express Signal | B | 0.35 D-GN | 2074 | Sunroof Switch Express Signal
C | 0.35 OG/BK | 144 | Sunroof Switch Open Vent Signal | C | 0.35 OG/BK | 144 | Sunroof Switch Open Vent Signal
D | 0.35 D-BU | 128 | Low Reference | D | 0.35 D-BU | 128 | Low Reference
E | 1 YE | 643 | Ignition Voltage | E | 0.8 YE | 643 | Ignition Voltage
F | 0.8 BK | 850 | Ground | F | 0.8 BK | 550 | Ground
G-H | -- | -- | Not Used | G-H | -- | -- | Not Used

### X400 Body Harness to the Chassis Harness

#### Connector Part Information

- OEM: 7283-5946-30
- Service: 88988239
- Description: 10-Way F YESC/USCAR Class III Series, Sealed (BK)

#### Connector Part Information

- OEM: 7282-5946-30
- Service: See Catalog
- Description: 10-Way M YESC/USCAR Class III Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 7116-4102-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

#### Terminal Part Information

- Pins: 2-4, 6-9
- Terminal/Tray: 7114-4102-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-3 (GY)

- Pins: 1, 10
- Terminal/Tray: 7114-4103-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-3 (GY)

#### X400 Body Harness to the Chassis Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.8 BK | 850 | Ground | 1 | 0.5 BK | 850 | Ground
2 | 0.35 L-BU | 5986 | Serial Data Communication Enable | 2 | 0.5 L-BU | 5986 | Serial Data Communication Enable
3 | 0.5 TN | 884 | Left Rear Wheel Speed Sensor Signal | 3 | 0.5 TN | 884 | Left Rear Wheel Speed Sensor Signal
4 | 0.5 OG | 885 | Low Reference | 4 | 0.5 OG | 885 | Low Reference
5 | -- | -- | Not Used | 5 | -- | -- | Not Used
6 | 0.5 TN/BK | 2500 | High Speed GMLAN Serial Data Bus+ | 6 | 0.5 TN/BK | 2500 | High Speed GMLAN Serial Data Bus+
7 | 0.5 TN | 2501 | High Speed GMLAN Serial Data Bus- | 7 | 0.5 TN | 2501 | High Speed GMLAN Serial Data Bus-
8 | 0.5 BN | 882 | Right Rear Wheel Speed Sensor Signal | 8 | 0.5 BN | 882 | Right Rear Wheel Speed Sensor Signal
9 | 0.5 WH | 883 | Low Reference | 9 | 0.5 WH | 883 | Low Reference
10 | 0.8 RD/WH | 1740 | Battery Positive Voltage | 10 | 0.5 RD/WH | 1740 | Battery Positive Voltage

### X403 Body Harness to the Left Tail Lamp Harness

#### Connector Part Information

- OEM: 6189-0319
- Service: 88988448
- Description: 6-Way F 090 Series, Sealed (L-GY)

#### Connector Part Information

- OEM: 6188-0173
- Service: See Catalog
- Description: 6-Way M TS 090 Series Sealed (L-GY)

#### Terminal Part Information

- Pins: 1
- Terminal/Tray: 7116-4026/11
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 15313892/J-35616-18 (BK)

- Pins: 2, 4, 5-6
- Terminal/Tray: 7116-4025/11
- Core/Insulation Crimp: Pins: 4 : E/A
- Core/Insulation Crimp: Pins: 2, 5-6 : E/1
- Release Tool/Test Probe: 15313892/J-35616-18 (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair K

#### X403 Body Harness to the Left Tail Lamp Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.8 YE | 18 | Left Rear Stop/Turn Lamp Control | 1 | 0.8 WH | 18 | Left Rear Stop/Turn Lamp Control
2 | 0.5 BK | 550 | Ground | 2 | 0.5 BK | 550 | Ground
3 | -- | -- | Not Used | 3 | -- | -- | Not Used
4 | 0.35 PU | 709 | Left Park Lamp Control | 4 | 0.35 D-GN | 709 | Left Park Lamp Control
5 | 0.5 L-BU | 20 | Stop Lamp Control | 5 | 0.5 D-BU | 20 | Stop Lamp Control/Stop Lamp Switch Signal
6 | 0.5 L-GN | 24 | Backup Lamp Control | 6 | 0.8 L-GN | 24 | Backup Lamp Control

### X404 Body Harness to the Right Tail Lamp Harness

#### Connector Part Information

- OEM: 6189-0319
- Service: 88988448
- Description: 6-Way F 090 Series, Sealed (L-GY)

#### Connector Part Information

- OEM: 6188-0173
- Service: See Catalog
- Description: 6-Way M TS 090 Series Sealed (L-GY)

#### Terminal Part Information

- Pins: 1
- Terminal/Tray: 7116-4026/11
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 15313892/J-35616-18 (BK)

- Pins: 2, 4, 5-6
- Terminal/Tray: 7116-4025/11
- Core/Insulation Crimp: Pins: 4 : E/A
- Core/Insulation Crimp: Pins: 2, 5-6 : E/1
- Release Tool/Test Probe: 15313892/J-35616-18 (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X404 Body Harness to the Right Tail Lamp Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.8 D-GN | 19 | Right Rear Stop/Turn Lamp Control | 1 | 0.8 WH | 19 | Right Rear Stop/Turn Lamp Control
2 | 0.5 BK | 850 | Ground | 2 | 0.35 BK | 850 | Ground
3 | -- | -- | Not Used | 3 | -- | -- | Not Used
4 | 0.35 BN/WH | 309 | Right Park Lamp Control | 4 | 0.35 D-GN | 309 | Right Park Lamp Control
5 | 0.5 L-BU | 20 | Stop Lamp Control | 5 | 0.5 D-BU | 20 | Stop Lamp Control/Stop Lamp Switch Signal
6 | 0.5 L-GN | 24 | Backup Lamp Control | 6 | 0.8 L-GN | 24 | Backup Lamp Control

### X406 Body Harness to the Fuel Sender Harness

#### Connector Part Information

- OEM: 12065425
- Service: 12125676
- Description: 10-Way F Metri-Pack 150 Series, Sealed (BK)

#### Connector Part Information

- OEM: 12048253
- Service: 12117372
- Description: 10-Way M Metri-Pack 150 Series Sealed (BK)

#### Terminal Part Information

- Pins: C, E, F, G, H, J, K, A, B
- Terminal/Tray: 12048074/2
- Core/Insulation Crimp: Pins: C, E, F, G, H, J, K : E/1
- Core/Insulation Crimp: Pins: A, B : 2/1
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X406 Body Harness to the Fuel Sender Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.5 WH | 1310 | EVAP Canister Vent Solenoid Control | 1 | 0.5 WH | 1310 | EVAP Canister Vent Solenoid Control
2 | 0.5 RD/WH | 2840 | Battery Positive Voltage | 2 | 0.5 PK | 2840 | Battery Positive Voltage
3 | 0.35 TN | 2759 | Low Reference | 3 | 0.35 BK/WH | 2759 | Low Reference
4 | 0.5 TN | 2759 | Low Reference | 4 | 0.35 BK | 2759 | Low Reference
5 | 0.5 D-GN | 890 | Fuel Tank Pressure Sensor Signal | 5 | 0.5 D-GN | 890 | Fuel Tank Pressure Sensor Signal
7 | 1.0 GY | 120 | Fuel Pump Control | 7 | 1.0 GY | 120 | Fuel Pump Control
8 | 1.0 BK | 850 | Ground | 8 | 0.8 BK | 850 | Ground
9 | 0.35 PU | 1589 | Fuel Level Sensor Signal | 9 | 0.35 PU | 1589 | Fuel Level Sensor Signal
10 | -- | -- | Not Used | 10 | 0.35 L-BU | 30 | Fuel Level Sensor Signal
11 | 0.5 GY | 2709 | 5-Volt Reference | 11 | 0.5 GY | 2709 | 5-Volt Reference

### X409 Body Harness to the Trailer Jumper Harness (V92)

#### Connector Part Information

- OEM: 7283-5889
- Service: See Catalog
- Description: 4-Way F 1.5 Sealed (BK)

#### Connector Part Information

- OEM: 72825889
- Service: See Catalog
- Description: 4-Way M 1.5 Sealed (BK)

#### Terminal Part Information

- Pins: 1-3
- Terminal/Tray: 7116-4102-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

- Pins: 4
- Terminal/Tray: 7116-4103-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

#### Terminal Part Information

- Pins: 1-3
- Terminal/Tray: 7114-4102-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-3 (GY)

#### X409 Body Harness to the Trailer Jumper Harness (V92)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.5 YE | 1618 | Trailer Left Rear Turn/Stop Lamp Control | 1 | 0.5 YE | 1618 | Trailer Left Rear Turn/Stop Lamp Control
2 | 0.5 D-GN | 1619 | Trailer Right Rear Turn/Stop Lamp Control | 2 | 0.5 D-GN | 1619 | Trailer Right Rear Turn/Stop Lamp Control
3 | 0.5 BN | 2109 | Trailer Park Lamps Control | 3 | 0.5 BN | 2109 | Trailer Park Lamps Control
4 | 1.0 BK | 550 | Ground | 4 | 1.0 BK | 850 | Ground

### X410 Trailer Harness to the Trailer Jumper Harness (V92)

#### Connector Part Information

- OEM: 72835889
- Service: See Catalog
- Description: 4-Way F 1.5 Sealed (BK)

#### Connector Part Information

- OEM: 72825889
- Service: See Catalog
- Description: 4-Way M 1.5 Sealed (BK)

#### Terminal Part Information

- Pins: 1-3Terminal/Tray: 7116-4102-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

- Pins: 4
- Terminal/Tray: 7116-4103-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

#### Terminal Part Information

- Pins: 1
- Terminal/Tray: 7114-4103-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-3 (GY)

- Pins: 2-4
- Terminal/Tray: 7114-4102-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-3 (GY)

#### X410 Trailer Harness to the Trailer Jumper Harness (V92)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 1.0 BK | 850 | Ground | 1 | 1.0 BK | 850 | Ground
2 | 0.5 BN | 2109 | Trailer Park Lamps Control | 2 | 0.5 BN | 2109 | Trailer Park Lamps Control
3 | 0.5 YE | 1618 | Trailer Left Rear Turn/Stop Lamp Control | 3 | 0.5 YE | 1618 | Trailer Left Rear Turn/Stop Lamp Control
4 | 0.5 D-GN | 1619 | Trailer Right Rear Turn/Stop Lamp Control | 4 | 0.5 D-GN | 1619 | Trailer Right Rear Turn/Stop Lamp Control

### X412 Headliner Harness to the Instrument Panel Harness (UUC)

#### Connector Part Information

- OEM: 7283-9078-80
- Service: See Catalog
- Description: 16-Way F Kaizen 0.64 Series (BN)

#### Connector Part Information

- OEM: 7282-9072-80
- Service: See Catalog
- Description: 16-Way M YESC Kaizen 0.64, Unsealed (BN)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Pins: A1- A2, A9-A11, B1-B3, B9-B11
- Terminal/Tray: 15304702/19
- Core/Insulation Crimp: E/4
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

- Pins: A5-A8, B5-B8
- Terminal/Tray: 15304722/8
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-5 (PU)

#### X412 Headliner Harness to the Instrument Panel Harness (UUC)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.5 WH | 1487 | Antenna Enable Signal | 1 | 0.5 WH | 1487 | Antenna Enable Signal
2 | 0.5 BARE | 6980 | DVD Audio Shield | 2 | 0.35 BARE | 6980 | DVD Audio Shield
3 | 0.5 L-BU | 5826 | Left DVD Audio Signal (+) | 3 | 0.5 L-BU | 5826 | Left DVD Audio Signal (+)
4 | 0.5 PU | 6979 | DVD Audio Common | 4 | 0.5 PU | 6979 | DVD Audio Common
5 | 0.5 WH | 5828 | Right DVD Audio Signal (+) | 5 | 0.5 WH | 5828 | Right DVD Audio Signal (+)
6 | 0.5 BARE | 6976 | DVD Video Drain Wire | 6 | 0.35 BARE | 6976 | DVD Video Drain Wire
7 | 0.5 D-GN | 6975 | DVD Video Signal (+) | 7 | 0.5 D-GN | 6975 | DVD Video Signal (+)
8 | 0.5 WH/BK | 5335 | DVD Video Signal (-) | 8 | 0.5 WH/BK | 5335 | DVD Video Signal (-)
9 | 0.5 TN/WH | 5830 | Remote Infra Red Signal (-) | 9 | 0.5 TN/WH | 5830 | Remote Infra Red Signal (-)
10 | 0.5 OG/BK | 5831 | Remote Infra Red Signal (+) | 10 | 0.5 OG/BK | 5831 | Remote Infra Red Signal (+)
11 | 0.35 YE | 343 | Ignition Voltage | 11 | 0.35 YE | 343 | Ignition Voltage
12 | 0.5 BN/WH | 5846 | Video Power Mode Signal | 12 | 0.5 BN/WH | 5846 | Video Power Mode Signal
13 | -- | -- | Not Used | 13 | -- | -- | Not Used
14 | 0.5 PK/BK | 5844 | Video Bright Control | 14 | 0.5 PK/BK | 5844 | Video Bright Control
15 | 0.5 BK/WH | 1551 | Ground | 15 | 0.5 BK/WH | 1551 | Ground
16 | 0.5 RD/WH | 2340 | Battery Positive Voltage | 16 | 0.5 RD/WH | 2340 | Battery Positive Voltage

### X415 Headliner Harness to the Body Harness

#### Connector Part Information

- OEM: 7283-3441-40
- Service: See Catalog
- Description: 8-Way F Kaizen YESC Series (L-GY)

#### Connector Part Information

- OEM: 7282-3441-40
- Service: See Catalog
- Description: 8-Way M Kaizen YESC Series (L-GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Pins: 2-5, 7
- Terminal/Tray: 7114-4101-08/9
- Core/Insulation Crimp: Pins: 5 : C/A
- Core/Insulation Crimp: Pins: 2-4, 7 : E/A
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

- Pins: 6
- Terminal/Tray: 7114-4100-08/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

#### X415 Headliner Harness to the Body Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | -- | -- | Not Used | 1 | -- | -- | Not Used
2 | 0.8 OG | 1732 | Courtesy Lamps Control | 2 | 0.8 OG | 1732 | Courtesy Lamps Control
3 | 0.8 BK | 850 | Ground (CF5) | 3 | 0.8 BK | 850 | Ground
4 | 0.8 BK | 850 | Ground | 4 | 0.8 BK | 850 | Ground
5 | 1.0 YE | 643 | Ignition Voltage | 5 | 1.0 YE | 643 | Ignition Voltage (CF5/DD7/DD8)
6 | 0.8 L-GN | 24 | Backup Lamp Control | 6 | 0.5 L-GN | 24 | Backup Lamp Control (DD7/DD8)
7 | 0.8 D-BU/WH | 149 | Courtesy Lamp Control | 7 | 0.8 D-BU/WH | 149 | Courtesy Lamp Control
8 | -- | -- | Not Used | 8 | -- | -- | Not Used

### X417 Headliner Harness to the Body Harness (U3U)

#### Connector Part Information

- OEM: 7283-6387-40
- Service: See Catalog
- Description: 6-Way F 0.64 Series (L-GY)

#### Connector Part Information

- OEM: 7282-6561-40
- Service: See Catalog
- Description: 6-Way M 0.64 Series (L-GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X417 Headliner Harness to the Body Harness (U3U)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1-4 | -- | -- | Not Used | 1-4 | -- | -- | Not Used
5 | 0.5 YE | 655 | Cellular Microphone Signal | 5 | 0.5 GY | 655 | Cellular Microphone Signal
6 | 0.5 BARE | 1489 | Drain Wire | 6 | 0.35 BARE | 1489 | Drain Wire

### X419 Body Harness to the Rear HVAC Harness (C69)

#### Connector Part Information

- OEM: 15326110
- Service: 15306171
- Description: 12-Way F 280 GT Series (BK)

#### Connector Part Information

- OEM: 15326942
- Service: 15326942
- Description: 12-Way M GT 280 Series (BK)

#### Terminal Part Information

- Pins: A-C, F-H, J-L
- Terminal/Tray: 15304711/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

- Pins: D, E
- Terminal/Tray: 15304713/19
- Core/Insulation Crimp: 4/4
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X419 Body Harness to the Rear HVAC Harness (C69)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.35 BN | 6555 | Rear Temperature Motor Control | A | 0.35 BN | 6555 | Rear Temperature Motor Control
B | 0.35 GY | 2614 | Auxiliary Air Temperature Door Control | B | 0.35 GY | 2614 | Auxiliary Air Temperature Door Control
C | 0.35 L-GN/WH | 5729 | Rear Mode Motor Control | C | 0.35 L-GN/WH | 5729 | Rear Mode Motor Control
D | 2.0 BK | 550 | Ground | D | 2.0 BK | 550 | Ground
E | 2.0 RD/WH | 2640 | Battery Positive Voltage | E | 2.0 RD/WH | 2640 | Battery Positive Voltage
F | 0.35 GY | 596 | 5-Volt Reference | F | 0.35 GY | 596 | 5-Volt Reference
G | 0.35 GY/BK | 754 | Blower Motor Speed Control | G | 0.35 D-GN | 2211 | Auxiliary Blower Motor Speed Control
H | 0.35 GY | 2599 | Auxiliary Mode Door Control | H | 0.35 GY | 2599 | Auxiliary Mode Door Control
J | 0.35 PK | 2145 | Air Temperature Switch Signal - Right | J | 0.35 PK | 2145 | Air Temperature Switch Signal - Right
K | 0.35 OG | 2215 | Auxiliary Mode Door Control | K | 0.35 OG | 2215 | Auxiliary Mode Door Control
L | 0.35 GY/BK | 1798 | Low Reference | L | 0.35 GY/BK | 1798 | Low Reference
M | -- | -- | Not Used | M | -- | -- | Not Used

### X420 Body Harness to the Left Inflatable Restraint Roof Rail Module Harness (ASF)

#### Connector Part Information

- OEM: 12077921
- Service: See Catalog
- Description: 2-Way F Metri-Pack 280 Series (YE)

#### Connector Part Information

- OEM: 12186799
- Service: See Catalog
- Description: 2-Way M 280 Series (YE)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X420 Body Harness to the Left Inflatable Restraint Roof Rail Module Harness (ASF)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.5 D-GN | 2137 | Side Impact Module - Left Front - High Control | A | 0.5 BN | 2137 | Side Impact Module - Left Front - High Control
B | 0.5 WH | 2138 | Side Impact Module - Left Front - Low Control | B | 0.5 YE/BK | 2138 | Side Impact Module - Left Front - Low Control

### X421 Body Harness to the Right Inflatable Restraint Roof Rail Module Harness (ASF)

#### Connector Part Information

- OEM: 12077921
- Service: See Catalog
- Description: 2-Way F Metri-Pack 280 Series (YE)

#### Connector Part Information

- OEM: 12186799
- Service: See Catalog
- Description: 2-Way M 280 Series (YE)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X421 Body Harness to the Right Inflatable Restraint Roof Rail Module Harness (ASF)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.5 D-GN | 2135 | Side Impact Module - Right Front - High Control | A | 0.5 TN/WH | 2135 | Side Impact Module - Right Front - High Control
B | 0.5 WH | 2136 | Side Impact Module - Right Front - Low Control | B | 0.5 L-GN | 2136 | Side Impact Module - Right Front - Low Control

### X500 Body Harness to the Left Front Door Harness

#### Connector Part Information

- OEM: 7183-1584
- Service: See Catalog
- Description: 28-Way F 090 Class II Series, Sealed (WH)

#### Connector Part Information

- OEM: 7182-1581
- Service: See Catalog
- Description: 28-Way M 090 Class II Series Sealed (WH)

#### Terminal Part Information

- Pins: 7-12, 19, 21
- Terminal/Tray: 7116-4020/11
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-18 (BK)

- Pins: 3-4, 23-24
- Terminal/Tray: 7116-4021/11
- Core/Insulation Crimp: Pins: 23-24 : 2/A
- Core/Insulation Crimp: Pins: 3-4 : E/A
- Release Tool/Test Probe: 15315247/J-35616-18 (BK)

- Pins: 25, 26
- Terminal/Tray: 7116-4022/11
- Core/Insulation Crimp: 4/A
- Release Tool/Test Probe: 15315247/J-35616-18 (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X500 Body Harness to the Left Front Door Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1-2 | -- | -- | Not Used | 1-2 | -- | -- | Not Used
3 | 0.8 GY | 118 | Left Front Speaker Output (-) | 3 | 0.35 TN | 118 | Left Front Speaker Output (-)
4 | 0.8 TN | 201 | Left Front Speaker Output (+) | 4 | 0.8 GY | 201 | Left Front Speaker Output (+)
5-6 | -- | -- | Not Used | 5-6 | -- | -- | Not Used
7 | 0.35 OG/BK | 781 | Driver Door Lock Switch Unlock Signal | 7 | 0.5 OG/BK | 781 | Driver Door Lock Switch Unlock Signal
8 | 0.35 PK/BK | 780 | Driver Door Lock Switch Lock Signal | 8 | 0.5 RD/BK | 780 | Driver Door Lock Switch Lock Signal
9 | 0.35 L-GN | 1499 | Driver Mirror Motor Left/Down Control | 9 | 0.35 YE | 1499 | Driver Mirror Motor Left/Down Control
10 | 0.35 BK/WH | 651 | Ground | 10 | 0.35 BK | 651 | Ground
11 | 0.35 YE | 88 | Driver Mirror Motor Up Control | 11 | 0.5 L-GN | 88 | Driver Mirror Motor Up Control
12 | 0.35 WH | 81 | Driver Mirror Motor Right Control | 12 | 0.5 WH | 81 | Driver Mirror Motor Right Control
13 | -- | -- | Not Used | 13 | 0.35 BK | 746 | Left Front Door Ajar Switch Signal
14-18 | -- | -- | Not Used | 14-18 | -- | -- | Not Used
19 | 0.35 GY/BK | 745 | Left Front Door Ajar Switch Signal | 19 | 0.5 RD/BK | 745 | Left Front Door Ajar Switch Signal
20 | -- | -- | Not Used | 20 | 0.35 PU | 294 | Not Used
21 | 0.35 BK/WH | 651 | Ground | 21 | 0.35 OG | 651 | Ground
22 | -- | -- | Not Used | 22 | -- | -- | Not Used
23 | 1.0 GY | 295 | Door Lock Actuator Lock Control | 23 | 1.0 GY | 295 | Door Lock Actuator Lock Control
24 | 1.0 TN | 694 | Driver Door Lock Actuator Unlock Control | 24 | 0.5 TN | 694 | Driver Door Lock Actuator Unlock Control
25 | 2.0 D-BU | 164 | Power Window Motor Left Front Up Control | 25 | 2.0 D-BU | 164 | Power Window Motor Left Front Up Control
26 | 2.0 BN | 165 | Power Window Motor Left Front Down Control | 26 | 2.0 BN | 165 | Power Window Motor Left Front Down Control
27-28 | -- | -- | Not Used | 27-28 | -- | -- | Not Used

### X600 Body Harness to the Right Front Door Harness

#### Connector Part Information

- OEM: 7183-1584
- Service: See Catalog
- Description: 28-Way F 090 Class II Series, Sealed (WH)

#### Connector Part Information

- OEM: 7182-1581
- Service: See Catalog
- Description: 28-Way M 090 Class II Series Sealed (WH)

#### Terminal Part Information

- Pins: 7-9, 11-13, 21, 23
- Terminal/Tray: 7116-4020/11
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-18 (BK)

- Pins: 3-4, 10, 20
- Terminal/Tray: 7116-4021/11
- Core/Insulation Crimp: Pins: 10, 20 : 2/A
- Core/Insulation Crimp: Pins: 3-4 : E/A
- Release Tool/Test Probe: 15315247/J-35616-18 (BK)

- Pins: 25-26
- Terminal/Tray: 7116-4022/11
- Core/Insulation Crimp: 4/A
- Release Tool/Test Probe: 15315247/J-35616-18 (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X600 Body Harness to the Right Front Door Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1-2 | -- | -- | Not Used | 1-2 | -- | -- | Not Used
3 | 0.8 D-GN | 117 | Right Front Speaker Output (-) | 3 | 0.8 TN | 117 | Right Front Speaker Output (-)
4 | 0.8 L-GN | 200 | Right Front Speaker Output (+) | 4 | 0.8 GY | 200 | Right Front Speaker Output (+)
5-6 | -- | -- | Not Used | 5-6 | -- | -- | Not Used
7 | 0.35 D-BU | 245 | Passenger Door Lock Switch Unlock Control | 7 | 0.5 OG/BK | 245 | Passenger Door Lock Switch Unlock Signal
8 | 0.35 L-BU | 244 | Passenger Door Lock Switch Lock Control | 8 | 0.5 RD/BK | 244 | Passenger Door Lock Switch Lock Signal
9 | 0.35 L-BU/WHT | 1497 | Passenger Mirror Motor Left/Down Control | 9 | 0.5 YE | 1497 | Passenger Mirror Motor Left/Down Control
10 | 1.0 GY | 295 | Door Lock Actuator Lock Control | 10 | 1.0 BK | 295 | Door Lock Actuator Lock Control
11 | 0.35 PU/WH | 889 | Passenger Mirror Motor Down Control | 11 | 0.5 L-GN | 889 | Passenger Mirror Motor Down Control
12 | 0.35 OG/WH | 881 | Passenger Mirror Motor Right Control | 12 | 0.5 WH | 881 | Passenger Mirror Motor Right Control
13 | 0.35 TN/WH | 746 | Right Front Door Ajar Switch Signal | 13 | 0.35 BK | 746 | Right Front Door Ajar Switch Signal
14-19 | -- | -- | Not Used | 14-18 | -- | -- | Not Used
19 | 0.35 RD/BK | 745 | Not Used
20 | 1.0 TN | 294 | Door Lock Actuator Unlock Control | 20 | 1.0 PU | 294 | Door Lock Actuator Unlock Control
21 | 0.35 BK/WH | 651 | Ground | 21 | 0.35 OG | 651 | Ground
22 | -- | -- | Not Used | 22 | -- | -- | Not Used
23 | 0.35 BK/WH | 651 | Ground | 23 | 0.35 GY | 651 | Ground
24 | -- | -- | Not Used | 24 | 0.35 TN | 694 | Not Used
25 | 2.0 L-BU | 166 | Power Window Master Switch Right Front Up Signal | 25 | 2.0 D-BU | 166 | Power Window Master Switch Right Front Up Signal
26 | 2.0 TN | 167 | Power Window Master Switch Right Front Down Signal | 26 | 2.0 BN | 167 | Power Window Master Switch Right Front Down Signal
27-28 | -- | -- | Not Used | 27-28 | -- | -- | Not Used

### X700 Body Harness to the Left Rear Door Harness

#### Connector Part Information

- OEM: 7123-1413
- Service: 88988485
- Description: 21-Way F (WH)

#### Connector Part Information

- OEM: 7122-1413
- Service: See Catalog
- Description: 21-Way M 0.070 Series (WH)

#### Terminal Part Information

- Pins: A1-A3
- Terminal/Tray: 7116-1050/27
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

- Pins: B5, B8, C2-C3, C6, C8
- Terminal/Tray: 173630-7/7
- Core/Insulation Crimp: Pins: B8, C2, C3, C8 : E/A
- Core/Insulation Crimp: Pins: B5, C6 : E/4
- Release Tool/Test Probe: 15315247/J-35616-33 (YE)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X700 Body Harness to the Left Rear Door Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A1 | 2.0 D-GN | 168 | Power Window Master Switch Left Rear Up Signal | A1 | 2.0 D-GN | 168 | Power Window Master Switch Left Rear Up Signal
A2 | 2.0 PU | 169 | Power Window Master Switch Left Rear Down Signal | A2 | 2.0 PU | 169 | Power Window Master Switch Left Rear Down Signal
A3 | 2.0 D-BU | 1307 | Power Window Master Switch Lockout Signal | A3 | 2.0 D-BU | 1307 | Power Window Master Switch Lockout Signal
B1-B4 | -- | -- | Not Used | B1-B4 | -- | -- | Not Used
B5 | 0.35 TN/WH | 746 | Right Front Door Ajar Switch Signal | B5 | 0.5 RD/BK | 746 | Right Front Door Ajar Switch Signal
B6 | -- | -- | Not Used | B6 | 0.35 BK | 746 | Not Used
B7 | -- | -- | Not Used | B7 | -- | -- | Not Used
B8 | 1.0 GY | 295 | Door Lock Actuator Lock Control | B8 | 1.0 GY | 295 | Door Lock Actuator Lock Control
B9 | -- | -- | Not Used | B9 | -- | -- | Not Used
C1 | -- | -- | Not Used | C1 | -- | -- | Not Used
C2 | 0.8 YE | 116 | Left Rear Speaker Output (-) | C2 | 0.8 BN | 116 | Left Rear Speaker Output (-)
C3 | 0.8 BN | 199 | Left Rear Speaker Output (+) | C3 | 0.8 YE | 199 | Left Rear Speaker Output (+)
C4 | -- | -- | Not Used | C4 | -- | -- | Not Used
C5 | -- | -- | Not Used | C5 | 0.35 PU | 294 | Not Used
C6 | 0.5 BK/WH | 651 | Ground | C6 | 0.35 BK | 651 | Ground
C7 | -- | -- | Not Used | C7 | -- | -- | Not Used
C8 | 1.0 TN | 294 | Door Lock Actuator Unlock Control | C8 | 1.0 TN | 294 | Door Lock Actuator Unlock Control
C9 | -- | -- | Not Used | C9 | -- | -- | Not Used

### X800 Body Harness to the Right Rear Door Harness

#### Connector Part Information

- OEM: 7123-1413
- Service: 88988485
- Description: 21-Way F (WH)

#### Connector Part Information

- OEM: 7122-1413
- Service: See Catalog
- Description: 21-Way M 0.070 Series (WH)

#### Terminal Part Information

- Pins: A1-A3
- Terminal/Tray: 7116-1050/27
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

- Pins: B6, B8, C2-C3, C5-C6
- Terminal/Tray: 173630-7/7
- Core/Insulation Crimp: Pins: C2-C3, C5-C6 : E/A
- Core/Insulation Crimp: Pins: B6, B8 : E/4
- Core/Insulation Crimp: Pins: :
- Release Tool/Test Probe: 15315247/J-35616-33 (YE)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X800 Body Harness to the Right Rear Door Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A1 | 2.0 L-GN | 170 | Power Window Master Switch Right Rear Up Signal | A1 | 2.0 D-GN | 170 | Power Window Master Switch Right Rear Up Signal
A2 | 2.0 PU | 171 | Power Window Master Switch Right Rear Down Signal | A2 | 2.0 PU | 171 | Power Window Master Switch Right Rear Down Signal
A3 | 2.0 D-BU | 1307 | Power Window Master Switch Lockout Signal | A3 | 2.0 D-BU | 307 | Headlamp Switch Flash to Pass Signal
B1-B4 | -- | -- | Not Used | B1-B4 | -- | -- | Not Used
B5 | -- | -- | Not Used | B5 | 0.5 RD/BK | 746 | Not Used
B6 | 0.35 TN/WH | 746 | Right Front Door Ajar Switch Signal | B6 | 0.35 BK | 746 | Right Front Door Ajar Switch Signal
B7 | -- | -- | Not Used | B7 | -- | -- | Not Used
B8 | 0.5 BK/WH | 651 | Ground | B8 | 0.35 GY | 651 | Ground
B9 | -- | -- | Not Used | B9 | -- | -- | Not Used
C1 | -- | -- | Not Used | C1 | -- | -- | Not Used
C2 | 0.8 L-BU | 115 | Right Rear Speaker Output (-) | C2 | 0.8 BN | 115 | Right Rear Speaker Output (-)
C3 | 0.8 D-BU | 46 | Right Rear Speaker Output (+) | C3 | 0.8 YE | 46 | Right Rear Speaker Output (+)
C4 | -- | -- | Not Used | C4 | -- | -- | Not Used
C5 | 1.0 TN | 294 | Door Lock Actuator Unlock Control | C5 | 1.0 PU | 294 | Door Lock Actuator Unlock Control
C6 | 1.0 GY | 295 | Door Lock Actuator Lock Control | C6 | 1.0 BK | 295 | Door Lock Actuator Lock Control
C7 | -- | -- | Not Used | C7 | -- | -- | Not Used
C8 | -- | -- | Not Used | C8 | 0.35 TN | 294 | Not Used
C9 | -- | -- | Not Used | C9 | -- | -- | Not Used

### X900 Body Harness to the Liftgate Harness

#### Connector Part Information

- OEM: 7283-6387-30
- Service: See Catalog
- Description: 6-Way F 064 Series (BK)

#### Connector Part Information

- OEM: 7282-6561-30
- Service: See Catalog
- Description: 6-Way M 064 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 7116-4720-02/14
- Core/Insulation Crimp: Pins: 1-3, 5-6 : H/H
- Core/Insulation Crimp: Pins: 4 : J/J
- Release Tool/Test Probe: 15315247/J-35616-64B (L-BU)

#### Terminal Part Information

- Pins: 1, 4
- Terminal/Tray: 7114-4721-02/14
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: 15315247/J-35616-65B (L-BU)

- Pins: 2-3, 5-6
- Terminal/Tray: 7114-4720-02/14
- Core/Insulation Crimp: J/J
- Release Tool/Test Probe: 15315247/J-35616-65B (L-BU)

#### X900 Body Harness to the Liftgate Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.35 PK/BK | 1303 | Liftgate Ajar Switch Signal | 1 | 0.5 PK/BK | 1303 | Liftgate Ajar Switch Signal
2 | 0.35 BN/WH | 309 | Right Park Lamp Control | 2 | 0.35 BN/WH | 309 | Right Park Lamp Control
3 | 0.35 GY | 391 | Rear Window Wiper Switch Signal | 3 | 0.35 GY | 391 | Rear Window Wiper Switch Signal
4 | 0.5 YE | 243 | Ignition Voltage | 4 | 0.5 YE | 243 | Ignition Voltage
5 | 0.35 L-GN | 2270 | Rear Window Washer Relay Control | 5 | 0.35 L-GN | 2270 | Rear Window Washer Relay Control
6 | 0.35 GY | 5797 | Rear Closure Handle Switch Open Signal | 6 | 0.35 GY | 5797 | Rear Closure Handle Switch Open Signal

### X901 Body Harness to the Liftgate Harness

#### Connector Part Information

- OEM: 7283-6466-40
- Service: See Catalog
- Description: 6-Way F Kaizen YESC Series (L-GY)

#### Connector Part Information

- OEM: 7282-6466-40
- Service: See Catalog
- Description: 6-Way M Kaizen YESC Series (L-GY)

#### Terminal Part Information

- Pins: 1, 5-6
- Terminal/Tray: 7116-4111-02/9
- Core/Insulation Crimp: C/A
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

- Pins: 3
- Terminal/Tray: 7116-4110-02/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

- Pins: 4
- Terminal/Tray: 7116-4112-02/9
- Core/Insulation Crimp: C/D
- Release Tool/Test Probe: 12094430/J-35616-35 (VT)

#### Terminal Part Information

- Pins: 1, 5-6
- Terminal/Tray: 7114-4111-02/9
- Core/Insulation Crimp: C/A
- Release Tool/Test Probe: 12094430/J-35616-5 (PU)

- Pins: 3
- Terminal/Tray: 7114-4110-02/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094430/J-35616-5 (PU)

- Pins: 4
- Terminal/Tray: 7114-4112-02/9
- Core/Insulation Crimp: C/D
- Release Tool/Test Probe: 12094430/J-35616-5 (PU)

#### X901 Body Harness to the Liftgate Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 1.0 BK | 550 | Ground | 1 | 1.0 BK | 550 | Ground
2 | -- | -- | Not Used | 2 | -- | -- | Not Used
3 | 0.5 L-BU | 6128 | Rear Closure Unlatch Motor Unlatch Control | 3 | 0.5 L-BU | 6128 | Rear Closure Unlatch Motor Unlatch Control
4 | 2.0 PU | 293 | Rear Defog Element Control | 4 | 2.0 BK | 293 | Rear Defog Element Control
5 | 1.0 BK | 550 | Ground | 5 | 1.0 BK | 550 | Ground
6 | 1.0 RD/WH | 2140 | Battery Positive Voltage | 6 | 1.0 RD/WH | 2140 | Battery Positive Voltage

### X906 Liftgate Harness to the License Lamp Harness

#### Connector Part Information

- OEM: 7283-5531-40
- Service: See Catalog
- Description: 6-Way F YESC/USCAR Class III Series (L-GY)

#### Connector Part Information

- OEM: 7282-5531-40
- Service: 88988483
- Description: 4-Way M YESC/USCAR Class III Series (L-GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Terminal/Tray: 7114-4100-08/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

#### X906 License Lamp Harness to the Liftgate Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.35 BK | 309 | Right Park Lamp Control | 1 | 0.35 BN/WH | 309 | Right Park Lamp Control
2 | 0.5 BK | 550 | Ground | 2 | 0.5 BK | 550 | Ground
3 | 0.35 L-GN | 5797 | Rear Closure Handle Switch Open Signal | 3 | 0.35 GY | 5797 | Rear Closure Handle Switch Open Signal
4 | 0.35 L-GN | 550 | Ground | 4 | 0.35 BK | 550 | Ground