For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the left rear trim panel. Refer to Quarter Lower Rear Trim Panel Replacement .
2. Remove the 3 auxiliary HVAC module mounting bolts. Refer to Auxiliary HVAC Module Replacement .
3. Reposition the auxiliary HVAC module inward to gain access to the blower control module.
4. Disconnect the electrical connection.

1 | Blower Control Module Screw (Qty: 2). Notice: Refer to Fastener Notice in the Preface section. Tighten 1.5 N·m (13 lb in)
2 | Blower Control Module Tip The blower control module is mounted on the outboard side of the module.