For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the left rear quarter lower trim panel. Refer to Quarter Lower Rear Trim Panel Replacement

1 | Digital Radio Receiver Nut (Qty: 4) Tighten 4 N·m (35 lb in)
2 | Digital Radio Receiver Assembly

#### Procedure

1. Disconnect the antenna and electrical connection.
2. Reprogram the digital radio receiver after replacement. Refer to Control Module References