For 1990-2009 cars

### Removal Procedure

1. Remove the push pins from the rear of the RH air inlet panel.
2. Open the hood.
3. Remove the push pins from the top and forward edge of the RH air inlet panel.
4. Remove the RH air inlet panel screw.
5. Remove the RH air inlet panel.
6. Remove the filter from the filter housing by depressing the release tab at the inboard edge of the filter housing.
7. Remove the filter from the vehicle.

### Installation Procedure

1. Install the filter to the vehicle.
2. Install the RH air inlet panel.
3. Install the RH air inlet panel screw.
4. Install the push pins to the top and forward edge of the RH air inlet panel.
5. Close the hood.
6. Install the push pins to the rear of the RH air inlet panel.