For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the dash panel heat shield nut.

Important: The heat shields at the dash panel and the catalytic converter overlap and utilizing common rivet attachment points.

3. Drill out the dash panel heat shield rivets.
4. Remove the dash panel heat shield.

### Installation Procedure

1. Position the dash panel heat shield to the underbody, installing the shield over the stud.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the dash panel heat shield nut.

Tighten
Tighten the nut to 10 N·m (89 lb in).

3. Install NEW rivets.
4. Lower the vehicle.