For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the rear seat. Refer to Rear Seat Replacement .
2. Loosen the seat back cover from the seat back filler panel. It is hooked into the slots of the panel.
3. Slide the rear seat back cover up the seat back enough to gain access to the seat back filler panel screws.

1 | Rear Seat No. 1 Back Panel Screw (Qty: 9) Notice: Refer to Fastener Notice in the Preface section. Tighten 9 N·m (80 lb in)
2 | Rear Seat No. 1 Back Panel