For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Open either the LF or RF door and the hood in order to access the molding assembly screws.

1 | Windshield Frame Filler Panel Applique Screw (Qty: 6) Notice: Refer to Fastener Notice in the Preface section. Tip One filler panel screw resides under the hood, open the hood in order to access the last filler panel screw. Tighten
1.9 N·m (17 lb in)

2 | Windshield Frame Filler Panel Applique Retainer (Qty: 11) Tip Release the integral retainers from the A-pillar.
3 | Windshield Frame Filler Panel Applique Nut (Qty: 5)