For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Raise the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the rear wheel and tire assembly. Refer to Tire and Wheel Removal and Installation .

1 | Adjustment Link to Knuckle Bolt and Nut Notice: Refer to Fastener Notice in the Preface section. Tighten 160 N·m (118 lb ft).
2 | Adjustment Link to Support Bolt and Nut Torque 160 N·m (118 lb ft).
3 | Adjustment Link Tip Check rear alignment. Refer to Wheel Alignment Measurement .