For 1990-2009 cars

### Removal Procedure

1. Remove the air cleaner assembly. Refer to Air Cleaner Assembly Replacement.
2. Remove the engine mount strut to bracket bolts (1).
3. Rotate the strut vertical.
4. Remove the engine mount strut bracket to cylinder head bolts (2).

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Position the engine mount strut bracket.
2. Install the engine mount strut bracket to cylinder head bolts (2).

Tighten
Tighten the nuts to 110 N·m (81 lb ft).

3. Install the engine mount strut bracket bolts (1).

Tighten
Tighten the bolts to 25 N·m (18 lb ft).

4. Install the air cleaner assembly. Refer to Air Cleaner Assembly Replacement.