For 1990-2009 cars

## Front Seat Head Restraint Guide Replacement Non Fold Flat

Callout | Component Name
--- | ---
1 | Front Seat Head Restraint Refer to Front Seat Head Restraint Replacement .
2 | Front Seat Head Restraint Guides

#### Procedure

1. Disconnect the lower J-hook retainer from the seat back trim cover.
2. Carefully pull up the trim cover, disengaging the hook and loop retainers, until the headrest guides are exposed.
3. Squeeze the locking tabs on the headrest guide and pull the guides up and out of the seat back pad.

## Front Seat Head Restraint Guide Replacement Fold Flat

Callout | Component Name
--- | ---
1 | Seat Back Cushion Finish Panel Refer to Driver Seat and Passenger Seat Back Cushion Finish Panel Replacement .
2 | Front Seat Head Restraint Refer to Front Seat Head Restraint Replacement .
3 | Front Seat Head Restraint Guides Tip Squeeze the bottom of the guides together and push upward to remove.