For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the rear seat. Refer to Rear Seat Replacement.
2. Remove the rear seat back cover and pad. Refer to Rear Seat Back Cushion Cover and Pad Replacement.
3. Remove the rear seat back release cables. Refer to Rear Seat Back Cushion Latch Cable Replacement.

1 | Rear Seat No. 1 Back Panel Screw (Qty: 9 Notice: Refer to Fastener Notice in the Preface section. Tighten 9N·m (80 lb in)
2 | Rear Seat No. 1 Back Panel
3 | Rear Seat No. 1 Back Frame Bolt (Qty: 4) Tighten 25N·m (18 lb ft)
4 | Rear Seat No. 1 Back Frame