For 1990-2009 cars

### Removal Procedure

1. Remove the rear side door window. Refer to Rear Side Door Window Replacement .
2. Remove the rear side door window weatherstrip run channel. Refer to Rear Side Door Window Weatherstrip Replacement .
3. Remove the bolts from the left and right sides.
4. Remove the screw from the upper corner.
5. Remove the rear side door window run channel and fixed window.

5.1. | Starting from the front corner of the door, remove the seal from the door header flange.

5.2. | Remove the seal from the door.

### Installation Procedure

1. Install the window run channel seal.

1.1. | Place the seal into the door frame.

1.2. | Place the seal on the door header.

1.3. | Install the seal to the door header flange, starting from the front corner.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the rear side door window run channel seal upper corner screw to the door frame.

Tighten
Tighten the nuts to 6 N·m (53 lb in).

3. Install the rear side window run channel seal bolts to the left and right sides.

Tighten
Tighten the nuts to 8 N·m (71 lb in).

4. Install the rear side door window weatherstrip run channel. Refer to Rear Side Door Window Weatherstrip Replacement .
5. Install the rear side door window. Refer to Rear Side Door Window Replacement .