For 1990-2009 cars

### Removal Procedure

1. Remove the front door upper trim panel extension. Refer to Front Side Door Trim Panel Replacement .
2. Disconnect the mirror electrical connector, if equipped.
3. Remove the mirror to door nuts.
4. Remove the mirror from the door.

### Installation Procedure

1. Position the mirror to the door.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the outside rearview mirror nuts.

Tighten
Tighten the nuts to 10 N·m (89 lb in).

3. Connect the electrical connector to the mirror, if equipped.
4. Inspect the operation of the mirror.
5. Install the front door upper trim panel extension. Refer to Front Side Door Trim Panel Replacement .