For 1990-2009 cars

### Removal Procedure

1. Remove the upper I/P trim panel. Refer to Instrument Panel Upper Trim Panel Replacement .
2. Remove the center air outlet duct push pins from the cross car beam.
3. Remove the center air outlet duct from the cross car beam.

### Installation Procedure

1. Inspect the seals, and replace if damaged, using Kent Industries adhesive backed foam tape P/N 46485 or equivalent.
2. Install the center air outlet duct to the cross car beam.
3. Install the center air outlet duct push pins to the cross car beam.
4. Install the upper I/P trim panel. Refer to Instrument Panel Upper Trim Panel Replacement .