For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the front seats. Refer to Front Seat Replacement - Bucket .

1 | Instrument Panel Lower Brace Bezel Refer to Instrument Panel Lower Brace Bezel Replacement .
2 | Console Screw (Qty: 2) Notice: Refer to Fastener Notice in the Preface section. Tighten 2 N·m (18 lb in)
3 | Console Bolt Cover (Qty: 4)

#### Procedure

Use a flat-bladed plastic trim tool to remove the covers.

4 | Console Bolt (Qty: 6) Tighten 9 N·m (80 lb in)
5 | Console Assembly

#### Procedures

1. Pull the parking brake lever up to the fully engaged position.
2. Disconnect the electrical connections to the console assembly.
3. With the aid of an assistant remove the console from the vehicle.