For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the front seat belt adjuster cover.
2. Remove seat belt guide loop bolt. Refer to Seat Belt Retractor Pretensioner Replacement - Front .
3. Remove the center pillar upper garnish molding. Refer to Center Pillar Upper Garnish Molding Replacement .

1 | Front Seat Belt Height Adjuster Bolt (Qty: 2) Notice: Refer to Fastener Notice in the Preface section. Tip Apply Permatex® 24200 on all restraint fasteners prior to installation. Tighten
40 N·m (30 lb ft)

2 | Front Seat Belt Height Adjuster Assembly