For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Disable the SIR system. Refer to SIR Disabling and Enabling .

1 | Windshield Side Garnish Molding Cover
2 | Windshield Side Garnish Screw Notice: Refer to Fastener Notice in the Preface section. Tighten 9 N·m (80 lb in)
3 | Windshield Garnish Molding Assembly

#### Procedure

Starting at the top, gently pull on the garnish molding to disengage the clip.

4 | Retainer Clip (Qty: 1)