For 1990-2009 cars

#### Tools Required

EN 46101 Spark Plug Tube Seal Guide

1. Install the EN 46101 onto the spark plug tubes of the left cylinder head.
2. Install the NEW camshaft cover bolt grommets prior to installing the camshaft cover bolts.
3. Wipe the camshaft cover sealing surface on the left cylinder head with a clean, lint-free cloth.
4. Place a bead 8 mm (0.3150 in) in diameter by 4 mm (0.1575 in) in height of RTV sealant, GM P/N 12378521 (Canadian P/N 88901148) or equivalent, on the engine front cover split lines (1).
5. Place the left camshaft cover into position onto the left cylinder head.
6. Loosely install the left camshaft cover bolts.

Notice: Refer to Fastener Notice in the Preface section.

7. Tighten the left camshaft cover bolts in the sequence shown.

Tighten

1. Tighten the left camshaft cover bolts in the sequence to 10 N·m (89 lb in).
2. Tighten the left camshaft cover bolts a second pass in the sequence to 10 N·m (89 lb in).

8. Remove the EN 46101 from the spark plug tubes of the left cylinder head.
9. Install the NEW spark plugs into the left cylinder head.

Tighten
Tighten the spark plugs to 20 N·m (15 lb ft).

10. Install the ignition coils.
11. Install the ignition coil bolts.

Tighten
Tighten the ignition coil bolts to 10 N·m (89 lb in).