For 1990-2009 cars

#### Heated Seat Module Scan Tool Data Parameters

Parameter | Expected Value | Definition
--- | --- | ---
Operating Conditions: Ignition ON
Driver Seat Heat Status | Inactive | The scan tool displays Active or Inactive. Active is displayed when the module commands seat heating ON.
Driver Seat HVC Level | Varies | The scan tool displays High, Medium or Low. This is the current level of seat heating as requested by the heated seat switch.
Driver Seat HVC Mode | Varies | The scan tool displays Off, Back & Cushion, Back Only, or Cool. This is the current mode of operation for the driver seat.
Passenger Seat Heat Status | Inactive | The scan tool displays Active or Inactive. Active is displayed when the module commands seat heating ON.
Passenger Seat HVC Level | Varies | The scan tool displays High, Medium or Low. This is the current level of seat heating as requested by the heated seat switch.
Passenger Seat HVC Mode | Varies | The scan tool displays Off, Back & Cushion, Back Only, or Cool. This is the current mode of operation for the passenger seat.
Seat Heat Supply Voltage | Inactive | The scan tool displays Active or Inactive. Active is displayed when the module commands seat heating ON.