For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the left rear trim panel. Refer to Quarter Lower Rear Trim Panel Replacement.
2. Remove the 3 auxiliary HVAC module mounting bolts. Refer to Auxiliary HVAC Module Replacement.
3. Reposition the auxiliary HVAC module inward to gain access to the blower control module.
4. Disconnect the electrical connection.

1 | Blower Control Module Screw (Qty: 2). Caution: Refer to Fastener Caution in the Preface section. Tighten 1.5 N·m (13 lb in)
2 | Blower Control Module Tip The blower control module is mounted on the outboard side of the module.