For 1990-2009 cars

Windshield wiper blades should be inspected for wear and cracking. See Scheduled Maintenance for more information.

Replacement blades come in different types and are removed in different ways. For proper type and length, see Maintenance Replacement Parts.

To replace the windshield wiper blade assembly:

1. Lift the wiper arm away from the windshield.
2. Push the release lever (B) to disengage the hook and push the wiper arm (A) out of the blade (C).
3. Push the new wiper blade securely on the wiper arm until you hear the release lever click into place.

To replace the rear window wiper blade:

1. Lift the wiper blade arm straight toward you.
2. Push the blade release button and slide the whole blade to the right to remove.
3. Install the new blade.
4. Push the wiper blade arm back into place.