For 1990-2009 cars

Callout | Component Name
--- | ---
Caution: When a hood hold open device is being removed or installed, provide alternate support to avoid the possibility of damage to the vehicle or personal injury.

#### Preliminary Procedures

1. Prop and support the hood.
2. Mark the location of the hinge to the hood with a grease pencil to aid in alignment.

1 | Hood Hinge Upper Bolts (Qty: 2) Notice: Refer to Fastener Notice in the Preface section. Tighten 25 N·m (18 lb ft)
2 | Hood Hinge Lower Bolts (Qty: 2) Tighten 25 N·m (18 lb ft)
3 | Hood Hinge