For 1990-2009 cars

## Liftgate Trim Panel Replacement Upper

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove lower liftgate trim panel. Refer to Liftgate Trim Panel Replacement.

1 | Liftgate Trim Panel Assembly Tip Pull away from liftgate to release retainers.
2 | Liftgate Trim Panel Retainer (Qty: 6)

## Liftgate Trim Panel Replacement Lower

Callout | Component Name
--- | ---
1 | Liftgate Trim Panel Screw (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
2 | Liftgate Trim Panel Nut (Qty: 2) Tighten 2 N·m (18 lb in)
3 | Liftgate Trim Panel Assembly Tip Pull away from liftgate to release retainers.
4 | Liftgate Trim Panel Retainer (Qty: 9)