For 1990-2009 cars

### Removal Procedure

1. Remove the air cleaner outlet duct. Refer to Air Cleaner Outlet Duct Replacement .
2. Disconnect the engine wiring harness electrical connector(s) (5) from the ignition coil(s).
3. Remove the ignition coil bolt(s).
4. Remove the ignition coil(s).

### Installation Procedure

1. Install the ignition coil(s).

Notice: Refer to Fastener Notice in the Preface section.

2. Install the ignition coil bolt(s).

Tighten
Tighten the bolt(s) to 10 N·m (89 lb in).

3. Connect the engine wiring harness electrical connector(s) (5) to the ignition coil(s).
4. Install the air cleaner outlet duct. Refer to Air Cleaner Outlet Duct Replacement .