For 1990-2009 cars

## Transmission Rear Mount Replacement FWD

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the right exhaust manifold. Refer to Exhaust Manifold Replacement - Right Side.
2. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
3. Support the transmission with a transmission jack.

1 | Rear Transmission Mount Thru Bolt Caution: Refer to Fastener Caution in the Preface section. Tighten 110 N·m (81 lb ft)
2 | Rear Transmission Mount Bolt (Qty: 3) Tighten 50 N·m (37 lb ft)
3 | Rear Transmission Mount

## Transmission Rear Mount Replacement AWD

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the right exhaust manifold. Refer to Exhaust Manifold Replacement - Right Side.
2. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
3. Support the transmission with a transmission jack.

1 | Rear Transmission Mount Thru Bolt Caution: Refer to Fastener Caution in the Preface section. Tighten 110 N·m (81 lb ft)
2 | Rear Transmission Mount Bolt Tighten 50 N·m (37 lb ft)
3 | Rear Transmission Mount