For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the knee bolster assembly. Refer to Knee Bolster Replacement .
2. Remove the instrument panel upper trim panel. Refer to Instrument Panel Upper Trim Panel Replacement .
3. Remove the left console trim panel. Refer to Front Floor Console Side Trim Panel Replacement - Left Side .
4. Remove the steering column trim panels. Refer to Steering Column Trim Covers Replacement .

1 | Lower Instrument Panel Trim Panel Assembly Screw (Qty: 7) Notice: Refer to Fastener Notice in the Preface section.

#### Procedure

Disconnect the electrical connections.

Tip
The left lower trim panel, center lower trim panel, and the cluster trim bezel are removed as an assembly.

Tighten
2 N·m (18 lb in)

2 | Retainer Clip (Qty: 2)
3 | Instrument Panel Lower Left Trim Panel Assembly Screw (Qty: 3). Tighten 2 N·m (18 lb in)
4 | Instrument Panel Lower Left Trim Panel Assembly

#### Procedure

If replacing the left lower trim panel, transfer all necessary components.