For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the front tire/wheel assembly. Refer to Tire and Wheel Removal and Installation .

1 | Rack And Pinion Outer Tie Rod End Nut Notice: Refer to Fastener Notice in the Preface section. Tighten 25 N·m (18 lb ft) plus 90 degrees
2 | Steering Gear Inner Tie Rod Nut

#### Procedure

1. Mark the location of the steering gear inner tie rod nut on the steering gear inner tie rod prior to loosening.
2. Loosen but do not remove the steering gear inner tie rod nut.

3 | Rack And Pinion Outer Tie Rod End

#### Procedure

1. Use puller J 24319-B to separate the rack and pinion outer tie rod end from the steering knuckle.
2. Inspect the steering gear inner tie rod for bent or damaged threads.
3. Clean the tapered surface of the steering knuckle.
4. Lubricate the steering gear inner tie rod threads with chassis lubricant. Refer to Fluid and Lubricant Recommendations .
5. Use installer J 44015 to install the rack and pinion outer tie rod end to the steering knuckle.
6. Remove installer J 44015 from the rack and pinion outer tie rod end.
7. Adjust the front toe. Refer to Front Toe Adjustment .

Tip
Do not free the rack and pinion outer tie rod end from the steering knuckle by use of a pickle fork or a wedge type tool. Damage to the seal or bushing may result.

Tighten
18 N·m (13 lb ft) plus 90 degrees

#### Special Tools

• | J 44015 Steering Linkage Installer

• | J 24319-B Steering Linkage and Tie Rod Puller