For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the instrument panel lower brace bezel. Refer to Instrument Panel Lower Brace Bezel Replacement .
2. Remove the console rear trim plate. Refer to Console Rear Trim Plate Replacement .

1 | Console Trim Plate Screw (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
2 | Console Trim Plate Assembly - Upper