For 1990-2009 cars

Callout | Component Name
--- | ---
Warning: In order to prevent SIR deployment, personal injury, or unnecessary SIR system repairs, do not strike the door or the door pillar in the area of the side impact sensor (SIS). Turn OFF the ignition and remove the key when performing service in the area of the SIS.
1 | Front Side Door Lock Striker Bolt (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 25 N·m (18 lb ft)
2 | Front Side Door Lock Striker Assembly Tip Ensure proper alignment after installation. Refer to Front Side Door Lock Striker Adjustment.
3 | Front Side Door Lock Striker Spacer