For 1990-2009 cars

### Removal Procedure

1. Remove the front side door window. Refer to Front Side Door Window Replacement .
2. Remove the front side door window weatherstrip run channel. Refer to Front Side Door Window Weatherstrip Replacement .
3. Remove the outside rearview mirror. Refer to Outside Rearview Mirror Replacement .
4. Remove the front door frame applique. Refer to Front Door Frame Applique Replacement .
5. Remove the front side door window run channel bolts.
6. Remove the front door window run channel. Starting from the rear corner of the door, remove the seal from the door header flange.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the front side door window run channel seal to the door header flange, starting from the rear corner.

Tighten
Tighten the bolts to 8 N·m (71 lb in).

2. Install the front side door window weatherstrip run channel. Refer to Front Side Door Window Weatherstrip Replacement .
3. Install the front door frame applique. Refer to Front Door Frame Applique Replacement .
4. Install the outside rearview mirror. Refer to Outside Rearview Mirror Replacement .
5. Install the front side door window. Refer to Front Side Door Window Replacement .