For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the front seat. Refer to Front Seat Replacement - Bucket.

1 | Front Seat Recliner Handle Tip Pull firmly forward on the handle to remove.
2 | Front Seat Outer Adjuster Finish Cover Refer to Front Seat Cushion Outer Trim Panel Replacement.
3 | Front Seat Belt Buckle Refer to Front Seat Belt Buckle Replacement.
4 | Front Seat Inner Adjuster Finish Panel Refer to Front Seat Cushion Inner Trim Panel Replacement.
5 | Front Seat Lumbar Support Actuator Knob Tip Remove the lumbar knob by pulling firmly on the knob.
6 | Front Seat Cushion Cover Refer to Front Seat Cushion Cover and Pad Replacement.
7 | Front Seat Heater Element Tip Disconnect the electrical connector and gently pull on the heater element to remove the element from the seat foam. Be careful not to damage the foam pad.