For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Raise the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the left wheel drive shaft. Refer to Front Wheel Drive Shaft Replacement .

1 | Left Front Wheel Drive Shaft Oil Seal Tip

• | For seal removal use J 6125-1B with J 23129 .

• | For seal installation use J 8092 with J-46629-A .

#### Special Tools

• | J 6125-1B Slide Hammer with Adapter

• | J 8092 Driver Handle

• | J 23129 Universal Seal Remover

• | J-46629-A Axle Seal Installer