For 1990-2009 cars

### Removal Procedure

Warning: Refer to Exhaust Service Warning in the Preface section.

Warning: Refer to Protective Goggles and Glove Warning in the Preface section.

1. Remove the exhaust manifold heat shield. Refer to Exhaust Manifold Heat Shield Replacement - Left Side .
2. Remove the oil level indicator. Refer to Oil Level Indicator and Tube Replacement .
3. Remove the catalytic converter to exhaust manifold nuts (1).
4. Remove the exhaust manifold bolts (1).

Note: Do not reuse the gasket.

5. Remove the exhaust manifold and gasket. Discard the gasket.

### Installation Procedure

1. Install one exhaust manifold bolt to the exhaust manifold.
2. Install the NEW exhaust manifold gasket onto the cylinder head and bolt.
3. Install the exhaust manifold (with gasket) to the catalytic converter and the cylinder head.

Caution: Refer to Fastener Caution in the Preface section.

4. Install the remaining exhaust manifold bolts (1) and tighten to 25 N·m (18 lb ft) .
5. Install the catalytic converter to exhaust manifold nuts (1) and tighten to 50 N·m (37 lb ft) .
6. Install the oil level indicator. Refer to Oil Level Indicator and Tube Replacement .
7. Install the exhaust manifold heat shield. Refer to Exhaust Manifold Heat Shield Replacement - Left Side .