For 1990-2009 cars

Scan Tool Parameter | Data List | Units Displayed | Typical Data Value
--- | --- | --- | ---
Operating Conditions: Ignition ON/Engine OFF/Vehicle Stationary for at Least 60 Minutes/Tire Pressures Adjusted to Recommended kPa/psi.
LF Pressure Status | Data Display | Unknown/Normal/Low/Flat/High | Normal
LF Pressure Sensor Mode | Data Display | Learn/Re-measure/Rolling/Entering Off/Exiting Off/Remeasure | Learn
LF Tire Pressure | Data Display | kPa/psi | 35 psi
LF Tire Pressure Sensor Battery Status | Data Display | OK/Low | OK
LF Tire Pressure, Sensor Status | Data Display | Normal/Failed | Normal
LR Pressure Status | Data Display | Unknown/Normal/Low/Flat/High | Normal
LR Pressure Sensor Mode | Data Display | Learn/Re-measure/Rolling/Entering Off/Exiting Off/Remeasure | Learn
LR Tire Pressure | Data Display | kPa/psi | 35 psi
LR Tire Pressure Sensor Battery Status | Data Display | OK/Low | OK
LR Tire Pressure, Sensor Status | Data Display | Normal/Failed | Normal
RF Pressure Status | Data Display | Unknown/Normal/Low/Flat/High | Normal
RF Pressure Sensor Mode | Data Display | Learn/Re-measure/Rolling/Entering Off/Exiting Off/Remeasure | Learn
RF Tire Pressure | Data Display | kPa/psi | 35 psi
RF Tire Pressure Sensor Battery Status | Data Display | OK/Low | OK
RF Tire Pressure, Sensor Status | Data Display | Normal/Failed | Normal/Failed
RR Pressure Status | Data Display | Unknown/Normal/Low/Flat/High | Normal
RR Pressure Sensor Mode | Data Display | Learn/Re-measure/Rolling/Entering Off/Exiting Off/Remeasure | Learn
RR Tire Pressure | Data Display | kPa/psi | 35 psi
RR Tire Pressure Sensor Battery Status | Data Display | OK/Low | OK
RR Tire Pressure, Sensor Status | Data Display | Normal/Failed | Normal
Learn in Progress | Data Display | Yes/No | No
Tire Pressure Indicator Requested | Data Display | Yes/No | No
TPM System Enabled | Data Display | Yes/No | Yes
Vehicle Speed Signal | Data Display | km/h/mph | 0