For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Video Display Assembly Screw (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tip The bolts have captured washers on them to keep them as part of the video display assembly, ensure that the washers are still on the assembly when reinstalling the display assembly.

Tighten
2 N·m (18 lb in)

2 | Video Display Assembly

#### Procedure

1. Pull down to disengage the retainer clip and remove from the vehicle.
2. Disconnect the electrical connector.